!
!
! ADTRAN, Inc. OS version 17.07.02.00
! Boot ROM version 17.04.01.00
! Platform: NetVanta 4430, part number 1700630E1
! Serial number!
!
hostname "_Primary2"
!
clock timezone -8
!
statistics rate-interval 30
!
ip subnet-zero
ip classless
ip routing
!
!
ip name-server 8.8.8.8 4.2.2.2
!
!
no auto-config
!
event-history on
event-history priority error
no logging forwarding
no logging email
!
service password-encryption
!
!
ip policy-timeout tcp telnet 14400
!
no ip firewall alg msn
no ip firewall alg mszone
no ip firewall alg h323
!
!
!
!
!
!
!
no dot11ap access-point-control
!
!
!
!
ip dhcp-server database local
!
ip dhcp-server pool "eth01"
  network 192.168.42.0 255.255.255.0
  default-router 192.168.42.1
!
!
!
!
!
!
!
no ethernet cfm
!
interface eth 0/1
  ip address  192.168.42.1  255.255.255.0
  shutdown
!
!
!
interface gigabit-eth 0/1
  description Up Stream
  encapsulation 802.1q
  no shutdown
!
interface gigabit-eth 0/1.318
  description Up Stream
  vlan-id 318
  ip address  46.10.233.227  255.255.255.248
  ip address  46.10.233.235  255.255.255.248  secondary
  ip address  46.10.249.52  255.255.255.240  secondary
  ip flow ingress
  vrrp 55 ip 46.10.233.226
  vrrp 55 ip 46.10.249.49 secondary
  vrrp 55 ip 46.10.233.234 secondary
  vrrp 55 priority 200
  no shutdown
!
interface gigabit-eth 0/2
  description Down Stream
  encapsulation 802.1q
  no shutdown
!
interface gigabit-eth 0/2.119
  vlan-id 119
  ip address  46.10.249.30  255.255.255.240
  ip address  46.184.148.78  255.255.255.240  secondary
  ip address  46.184.156.126  255.255.255.128  secondary
  ip address  43.119.205.60  255.255.255.248  secondary
  ip flow ingress
  vrrp 65 ip 46.10.249.17
  vrrp 65 ip 43.119.205.57 secondary
  vrrp 65 ip 46.184.156.1 secondary
  vrrp 65 ip 46.184.148.65 secondary
  vrrp 65 priority 200
  no shutdown
interface gigabit-eth 0/2.139
  vlan-id 139
  ip address  46.184.132.90  255.255.255.128
  ip address  10.0.0.1  255.255.255.0  secondary
  ip address  172.18.8.1  255.255.255.0  secondary
  ip flow ingress
  vrrp 65 ip 46.184.132.1
  vrrp 65 priority 200
  no shutdown
interface gigabit-eth 0/2.619
  vlan-id 619
  ip address  46.10.249.43  255.255.255.240
  ip address  46.184.148.30  255.255.255.224  secondary
  ip flow ingress
  vrrp 65 ip 46.10.249.33
  vrrp 65 ip 46.184.148.1 secondary
  vrrp 65 priority 200
  no shutdown
interface gigabit-eth 0/2.620
  vlan-id 620
  ip address  46.10.249.10  255.255.255.240
  ip address  46.184.148.62  255.255.255.224  secondary
  ip address  46.184.148.81  255.255.255.240  secondary
  ip address  46.184.149.1  255.255.255.252  secondary
  ip flow ingress
  vrrp 65 ip 46.10.249.1
  vrrp 65 ip 46.184.148.33 secondary
  vrrp 65 priority 200
  no shutdown
!
!
!
!
!
!
!
!
arp 46.184.156.8 00:1B:C0:53:36:06 arpa
arp 46.184.156.124 00:A0:C8:A5:38:C7 arpa
!
ip route 0.0.0.0 0.0.0.0 46.10.233.225
ip route 46.184.132.29 255.255.255.255 null 0
ip route 46.184.156.74 255.255.255.255 null 0
ip route 46.184.156.128 255.255.255.128 46.10.233.233
ip route 43.119.205.61 255.255.255.255 null 0
ip route 172.18.4.0 255.255.255.0 46.10.233.233
!
no ip tftp server
no ip tftp server overwrite
no ip http server
ip http secure-server 
no ip snmp agent
no ip ftp server
ip ftp server default-filesystem flash
no ip scp server
no ip sntp server
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
line con 0
  login
!
line telnet 0 4
  login local-userlist
  shutdown
line ssh 0 4
  login local-userlist
  no shutdown
!
sntp server time.nist.gov
sntp wait-time 500
!
!
!
!
end