!

!

! ADTRAN, Inc. OS version 17.09.01.00

! Boot ROM version 17.04.01.00

! Platform: NetVanta 4430, part number 1700630E1

! Serial number LBADTN1104AD536

!

!

hostname ""

!

clock timezone -6-Central-Time

!

ip subnet-zero

ip classless

ip routing

!

!

ip domain-proxy

ip name-server 10.10.1.250 4.2.2.1 4.2.2.2 10.59.1.1

!

!

no auto-config

!

event-history on

no logging forwarding

no logging email

!

service password-encryption

!

!

banner motd #

 Important

The ethernet 0/1 interface is enabled with an address of 10.10.10.1

Telnet/SSH access is also enabled.

#

!

ip policy-timeout tcp telnet 14400

!

no ip firewall alg msn

no ip firewall alg mszone

no ip firewall alg h323

!

!

!

!

!

!

!

no dot11ap access-point-control

!

!

!

!

!

!

!

qos map VoIP 10

 match precedence 5

 priority percent 90

qos map VoIP 20

 match precedence 3

 bandwidth remaining percent 10

!

!

!

ip flow top-talkers

!

!

no ethernet cfm

!

interface eth 0/1

 description LEC ID: 31HCGS689603

 no ip address

 no shutdown

!

!

!

interface gigabit-eth 0/1

 ip address \*\*\* 255.255.255.0

 ip address \*\*\* 255.255.255.0 secondary

 no shutdown

!

!

interface gigabit-eth 0/2

 no ip address

 shutdown

!

!

!

!

interface t1 3/1

 description LEC ID: 31HCGS689600

 tdm-group 1 timeslots 1-24 speed 64

 no shutdown

!

interface t1 3/2

 description LEC ID: 31HCGS689601

 tdm-group 1 timeslots 1-24 speed 64

 no shutdown

!

interface t1 3/3

 description LEC ID: 31HCGS689602

 tdm-group 1 timeslots 1-24 speed 64

 no shutdown

!

interface t1 3/4

 description LEC ID: 31HCGS689603

 tdm-group 1 timeslots 1-24 speed 64

 no shutdown

!

interface t1 3/5

 shutdown

!

interface t1 3/6

 shutdown

!

interface t1 3/7

 shutdown

!

interface t1 3/8

 shutdown

!

!

interface fr 1 point-to-point

 description fr 1

 frame-relay lmi-type cisco

 frame-relay multilink

 max-reserved-bandwidth 90

 qos-policy out VoIP

 no shutdown

 cross-connect 1 t1 3/1 1 frame-relay 1

 cross-connect 2 t1 3/2 1 frame-relay 1

 cross-connect 3 t1 3/3 1 frame-relay 1

 cross-connect 4 t1 3/4 1 frame-relay 1

!

interface fr 1.100 point-to-point

 frame-relay interface-dlci 100

 description fr 1.100

 ip address \*\*\*\* 255.255.255.252

 ip flow ingress

 ip flow egress

 media-gateway ip primary

 bandwidth 6144

 no lldp send-and-receive

!

!

!

!

router bgp 65130

 no auto-summary

 no synchronization

 network \*\*\* mask 255.255.255.0

 network \*\*\*\* mask 255.255.255.0

 neighbor \*\*\*

 no default-originate

 soft-reconfiguration inbound

 remote-as 65000

!

!

!

!

!

ip route 0.0.0.0 0.0.0.0 fr 1.100

!

no ip tftp server

no ip tftp server overwrite

ip http server

ip http secure-server

ip snmp agent

no ip ftp server

ip ftp server default-filesystem flash

no ip scp server

no ip sntp server

!

!

!

!

snmp-server contact ""

snmp-server contact phone ""

snmp-server contact email ""

snmp-server chassis-id ""

snmp-server enable traps snmp

snmp-server community

!

!

!

!

ip sip udp 5060

ip sip tcp 5060

!

!

!

!

!

!

!

!

!

!

!

!

!

!

ip domain-proxy source-interface gigabit-ethernet 0/1

!

line con 0

 no login

!

line telnet 0 4

 login

 password encrypted

 no shutdown

line ssh 0 4

 login local-userlist

 no shutdown

!

!

!

!

!

end