{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["AP Feature Matrix"],"not_rendered":{"charts":0,"images":23,"macros":1,"external_links":0,"defined_names":30,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"AP Feature Matrix","index":0,"n_rows":118,"n_cols":17,"rows_kept":118,"cut":false,"hidden":false,"merged":[]}
[null,"Updated: 02/13/2017\nFeature Support as of vWLAN Release 3.0.0\n•   Supported\n— Not Supported or Not Applicable\nŦ Restrictions Apply","BSAP 1920","BSAP 1925","BSAP 1930","BSAP 1935","BSAP 1940 \nOutdoor AP","BSAP 2020","BSAP 2030","BSAP 2035","BSAP 2135\nOutdoor AP","BSAP 3040","BSAP 3045","BSAP 1800 v2\n(Legacy Discontinued)","BSAP 1840\n(Legacy Discontinued)","NV 160\n(Legacy Discontinued)","NV 161\n(Legacy Discontinued)"]
[null,"Part Number","1700954F1","1700955F1","1700950F1","1700951F1","1700952F1","1700945F1","1700948F1 ","1700949F1 ","1700962F1","1700965F1","1700966F1","1700910F1","1700911F1","1700416F1","1700417F1"]
[null,"AP Type 802.11","A/B/G/N","A/B/G/N","A/B/G/N","A/B/G/N","A/B/G/N","A/B/G/N/AC","A/B/G/N/AC","A/B/G/N/AC","A/B/G/N/AC","A/B/G/N/WAVE2 AC","A/B/G/N/WAVE2 AC","A/B/G/N","A/B/G/N","A/B/G/N","A/B/G/N"]
[null,"Latest AP Firmware Release","2.9.0","2.9.0","2.9.0","2.9.0","2.9.0","2.9.0","2.9.0","2.9.0","2.9.0","3.0.0","3.0.0","2.9.0","2.9.0","6.9.2-2","6.9.2-2"]
[null,"Initial Controller Firmware Release","2.3.0.09","2.3.0.09","2.3.0.09","2.3.0.09","2.3.0.09","2.8.0","2.5.0.05 ","2.5.0.05 ","2.6.0.19","3.0.0","3.0.0","2.1.0.14","2.1.0.14","R10.4.0 ","R10.4.0 "]
[null,"Highest Supported Controller Firmware Release","2.9.0","2.9.0","2.9.0","2.9.0","2.9.0","2.9.0","2.9.0","2.9.0","2.9.0","3.0.0","3.0.0","2.9.0","2.9.0","R11.6.0.SA ","R11.6.0.SA "]
[null,"Controller Options"]
[null,"BlueSocket vWLAN ","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—"]
[null,"ProCloud Managed","•","•","•","•","•","•","•","•","•","•","•","—","—","—","—"]
[null,"NetVanta Controller (AWCP)","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•"]
[null,"Admin and Management"]
[null,"Auto-Discovery  ","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Captive Portal (Splashpage)","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Dashboard Branding {2.9.0}","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Job/Task Schedules {2.9.0}","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—"]
[null,"SAML 2.0 Single Sign On for Admin {2.8.0} ","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Zero IT Setup For ProCloud {R2.6.0}","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Features","`"]
[null,"Apple Bonjour Services","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Apple Captive Network Assistant (CNA)","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—"]
[null,"AP Sensor mode","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Beamforming","•","•","•","•","•","—","2.4Ghz only","2.4Ghz only","•","—","—","—","—","—","—"]
[null,"Band/Dynamic Steering {2.9.0}","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Dynamic RF Management {2.9.0}","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—"]
[null,"High Availabilty","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—"]
[null,"IPV6","Ŧ","Ŧ","Ŧ","Ŧ","Ŧ","Ŧ","Ŧ","Ŧ","Ŧ","Ŧ","Ŧ","—","—","—","—"]
[null,"Layer 2 & Layer 3 Tunneling","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Load Balancing","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Mesh / Bridging","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—"]
[null,"Microsoft Network Connectivity Status Indicator (NCSI)","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Multicast Rate Control","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Packet Aggregation:A-MPDU, A-MSDU","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Quality of Service (WMM, 802.11e)","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RADIUS-based MAC Authentication {R2.6.2}","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Rate Limiting","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Roaming (Layer 2)","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•"]
[null,"Roaming (Layer 3)","•","•","•","•","•","•","•","•","•","•","•","—","—","—","—"]
[null,"WMM (Wi-Fi Multimedia QoS), 802.11e","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"WMM Power Save (U-APSD)","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Performance"]
[null,"20 MHz and 40 MHz Channels","•","•","•","•","•","•","•","•","•","•","•","A/B/G/N","A/B/G/N","•","•"]
[null,"80 MHz Channels","—","—","—","—","—","•","•","•","•","•","•","•","•","—","—"]
[null,"80+80 MHz Channel  {R3.0.0}","—","—","—","—","—","—","—","—","—","•","•","—","—","—","—"]
[null,"802.11n MIMO support","2x2:2 ","2x2:2 ","3x3:3","3x3:3","3x3:3","2x2:2","3x3:3","3x3:3","3x3:3","4x4:4","4x4:4","2x3:2","2x3:2","2x3:2","2x3:2"]
[null,"802.11Wave2 AC MU-MIMO support {R3.0.0}","—","—","—","—","—","—","—","—","—","4x4:4","4x4:4"]
[null,"Theoretical Bandwidth ","300 Mbps / Radio\n600 Mbps / AP","300 Mbps / Radio\n600 Mbps / AP","450 Mbps /Radio\n900 Mbps / AP","450 Mbps /Radio\n900 Mbps / AP","450 Mbps /Radio\n900 Mbps / AP","450 Mbps / 2.4 GHz Radio\n1.3 Gbps / 5.8 GHz radio\n1.75 Gbps / AP","450 Mbps / 2.4 GHz Radio\n1.3 Gbps / 5.8 GHz radio\n1.75 Gbps / AP","450 Mbps / 2.4 GHz Radio\n1.3 Gbps / 5.8 GHz radio\n1.75 Gbps / AP","450 Mbps / 2.4 GHz Radio\n1.3 Gbps / 5.8 GHz radio\n1.75 Gbps / AP","800 Mbps / 2.4 GHz Radio\n1..733 Gbps / 5.8 GHz radio\n2.5 Gbps / AP","800 Mbps / 2.4 GHz Radio\n1..733 Gbps / 5.8 GHz radio\n2.5 Gbps / AP","300 Mbps / Radio\n600 Mbps / AP","300 Mbps / Radio\n600 Mbps / AP","300 Mbps / radio      600 Mbps / AP","300 Mbps / Radio\n600 Mbps / AP"]
[null,"Security"]
[null,"Rogue AP Detection","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Stateful Inspection Firewall","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Layer 7 Device Fingerprinting {R2.6.0}","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"WEP, WPA, WPA2 (AES & TKIP),\n802.11i, 802.1X, PSK","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Accessories"]
[null,"PoE Injectors"]
[null,"802.3af PoE Injector","P/N 1700926F1","P/N 1700926F1","P/N 1700926F1","P/N 1700926F1","—","P/N 1700926F1","P/N 1700926F1","P/N 1700926F1","—","—","—","P/N 1700920F1","P/N 1700920F1","P/N 1700920F1","P/N 1700920F1"]
[null,"802.3at Indoor PoE(+) Injector (1700923F1)","•","•","•","•","P/N 1700923F1","—","—","—","P/N 1700923F1","P/N 1700923F1","P/N 1700923F1","—","—","—","—"]
[null,"Power Adapters"]
[null,"12V DC Power Adapter (1700922F1)","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•"]
[null,"12V DC Power Adapter (1700928F1)","•","•","—","—","—","•","—","—","—","—","—","—","—","—","—"]
[null,"12V DC Power Adapter (1700929F1)","—","—","•","•","—","—","•","•","—","—","—","—","—","—","—"]
[null,"12V DC Power Adapter (1700963F1)","—","—","—","—","—","—","—","—","—","•","•","—","—","—","—"]
[null," Antennas Bundles"]
[null,"Antenna Bundle (1700930F1)","—","—","—","—","•","—","—","—","•","—","—","—","—","—","—"]
[null,"Antenna Bundle (1700931F1)","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Antenna Bundle (1700932F1)","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Antenna Bundle (1700957F1)","—","—","—","—","—","—","—","•","—","—","—","—","•","—","—"]
[null,"Antenna Bundle (1700964F1)","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—"]
[null,"Antenna Bundle (1700939F1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•"]
[null,"Mounting Kit"]
[null,"Recessed Ceiling Mount Kit (1700921F1)","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•"]
[null,"Mounting kit included:Desktop /wall /ceiling) ","•","•","•","•","—","•","•","•","—","•","•","•","•","•","•"]
[null,"Console Cable"]
[null,"AP Console Cable (1700924F1)","—","—","•","•","—","•","•","•","—","•","•","•","•","•","•"]
[null,"Physical Specifications"]
[null,"Antenna Type","Internal","4 External \nRP_SMA Connectors","Internal","6 External \nRP_SMA Connectors","6 External \nType N Connectors","Internal","Internal","6 External \nRP_SMA Connectors","6 External \nType N Connectors","Internal","8 External \nRP_SMA Connectors","Internal","6 External \nRP_SMA Connectors","Internal","6 External RP_SMA Connectors"]
[null,"BTU  ","TBD","TBD","TBD","TBD","TBD","TBD","TBD","TBD","TBD","TBD","TBD","TBD","TBD","TBD","TBD"]
[null,"Humidity 5% to 90% non-condensing","•","•","•","•","—","•","•","•","—","•","•","—","—","—","—"]
[null,"Humidity 15% to 95% non-condensing ","—","—","—","—","•","—","—","—","•","—","—","•","•","•","•"]
[null,"IP67 - Waterproof","—","—","—","—","•","—","—","—","•","—","—","—","—","—","—"]
[null,"Kensington Style Lock Feature","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Mean Time Between Failure (MTBF)","+500,000 hrs","+500,000 hrs","+500,000 hrs","601,343","TBD","TBD","TBD","TBD","TBD","TBD","TBD","TBD","TBD","606061","TBD"]
[null,"Operating Temperature °C","0°C to 45°C","0°C to 45°C","0°C to 50°C","0°C to 50°C","-40°C to 55°C","(0° C to 40° C)","0°C to 50°C","0°C to 50°C","-40°C to 55°C","0° C to 45° C","0° C to 45° C","-5°C to 55°C","-5°C to 55°C","-5°C to 55°C","-5°C to 55°C"]
[null,"Operating Temperature °F","32°F to 113°F","32°F to 113°F","32°F to 122°F","32°F to 122°F","-40°F to 122°F"," 32° F to 104° F","32° F to 122° F","32° F to 122° F","-40°F to 122°F","32° F to 113° F","32° F to 113° F","22°F to 131°F","22°F to 131°F","22°F to 131°F","22°F to 131°F"]
[null,"Plenum Rated","•","•","•","•","•","•","•","•","•","—","•","•","•","—","—"]
[null,"Salt-spray resistant","—","—","—","—","*","—","—","—","*","—","—","—","—","—","—"]
[null,"Warranty - Limited Lifetime","•","•","•","•","—","•","•","•","—","•","•","—","—","—","—"]
[null,"Warranty - One Year (Parts)","—","—","—","—","•","—","—","—","•","—","—","•","•","•","•"]
[null,"Weight",".44 lb (0.2kg)",".44 lb (0.2kg)","1.25 lb (0.6 kg)","1.25 lb (0.6 kg)","3.2 lb (1.45 kg)",".44 lb (0.2kg)","1.25 lbs (0.6 kg) ","1.25 lbs (0.6 kg) ","3.2 lb (1.45 kg)","1.5lbs (0.7 kg)","1.5lbs (0.7 kg)","2.0 lb (0.7kg)","1.5 lb (0.7kg)","2.0 lb (0.7kg)","1.5 lb (0.7kg)"]
[null,"Power "]
[null,"802.3af","•","•","•","•","—","•","•","•","—","—","—","•","•","•","•"]
[null,"802.3at (PoE+)","•","•","•","•","•","•","•","•","•","•","•","—","—","—","—"]
[null,"Max Power Consumption over POE","12W","12W","12W","12W","23W","12W","12W","12W","23W","23W","23W","11 W","11 W","11 W","11 W"]
[null,"Power Save (U-APSD)","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Transmit Power (Max)","100 mW","100 mW","100 mW","100 mW","50 mW UNII-1\n400 mW UNII-3","100 mW","100 mW","100 mW","50 mW UNII-1\n400 mW UNII-3","160 mW","160 mW","100 mW","100 mW","100 mW","100 mW"]
[null,"Dimensions"]
[null,"Dimensions in inches: (H x W x D)","Dia 6.3 x 1.5 H","Dia 6.3 x 1.5 H","1.5 x 6.5 x 6.5","1.5 x 6.5 x 6.5","1.9 x 7.8 x 9.6","Dia 6.3 x 1.5 H","1.5 x 6.5 x 6.5","1.5 x 6.5 x 6.5","1.9 x 7.8 x 9.6","8.3 x 8.3 x 1.5 ","8.3 x 8.3 x 1.5 ","2.1 x 7.8 x 7.8","1.8 x 7.8 x 7.8","2.1 x 7.8 x 7.8","1.8 x 7.8 x 7.8"]
[null,"Dimensions in mm: (H x W x D)","Dia 160 x 38 H","Dia 160 x 38 H","35 x 165 x 165","35 x 165 x 165","75 x 200 x 245","Dia 160 x 38 H","35 x 165 x 165","35 x 165 x 165","75 x 200 x 245","210 x 210 x 35","210 x 210 x 35","54 x 198 x 198","46 x 198 x 198","54 x 198 x 198","46 x 198 x 198"]
[null,"Compliance"]
[null,"Agency Approvals"]
[null,"CSA 22.2","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"EN 60950","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"IEC 60950","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RoHS Compliant","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"UL 1950 ","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Wi-Fi Certified","Certificate","Certificate","Certificate","•","•","•","•","•","•","•","•","Certificate","Certificate","—","—"]
[null,"DFS and 802.11h (Europe Only) {R2.6.0}","• HW Rev K","•","• HW Rev K","•","•","—","—","—","—","—","—","—","—","—","—"]
[null,"Radio Approvals"]
[null,"AS/NZS 3548","•","•","•","•","—","•","•","•","—","•","•","•","•","•","•"]
[null,"AS/NZS 44268/C-Tick (Australia & New Zealand)","—","—","—","—","•","—","—","—","•","—","—","—","—","—","—"]
[null,"AS/NZS 4771 (Australia & New Zealand)","•","•","•","•","—","•","•","•","—","•","•","•","•","•","•"]
[null,"EMI and Susceptibility (Class A)","•","•","•","•","—","•","•","•","—","•","•","•","•","•","•"]
[null,"EN 300.328 (Europe)","•","•","•","•","•","•","•","•","•","•","•",null,null,"•","•"]
[null,"EN 300.893 (Europe)","—","—","—","—","•","—","—","—","•","—","—","—","—","—","—"]
[null,"EN 301.489-1/-17 (Europe)","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"FCC Part 15.107 and 15.109","•","•","•","•","—","•","•","•","—","•","•","•","•","•","•"]
[null,"FCC Part 15.247","•","•","•","•","•","•","•","•","•","•","•",null,null,"•","•"]
[null,"ICES-003 (Canada)","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"NCC (Taiwan) and IDA (Singapore)","•","•","•","•","—","—","•","•","—","•","•","•","•","•","•"]
[null,"RSS-210 (Canada)","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]