{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["AOS Feature Matrix"],"not_rendered":{"charts":0,"images":28,"macros":1,"external_links":0,"defined_names":64,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"AOS Feature Matrix","index":0,"n_rows":462,"n_cols":41,"rows_kept":462,"cut":false,"hidden":false,"merged":[]}
[null,"Router/IPBG\nFeature Matrix\n\n      Updated: 11/18/22\n• Supported (IPv4 Unless noted)\n—Not Supported or Not Applicable\nŦ Restrictions Apply\nŦ Dependent upon specific build","NV3140","NV3148","NV4148","NV4305\n2nd Gen","NV4430","NV4660","NV5660","TA 900\n3rd Gen","TA 900e\n3rd Gen","NV6250","NV6330","NV6360","NV1224STR\nDiscontinued\n","NV1224R\nDiscontinued\n","NV1335\nDiscontinued\n","NV3120\nDiscontinued\n","NV3130\nDiscontinued\n","NV3200\n2nd Gen\nDiscontinued\n","NV3200\n3rd Gen\nDiscontinued\n","NV3205\n2nd Gen\nDiscontinued\n","NV3205\n3rd Gen\nDiscontinued\n","NV3305\n2nd Gen\nDiscontinued\n","NV3430\n1st Gen\nDiscontinued\n","NV3430\n2nd Gen\nDiscontinued\n","NV3448\nDiscontinued\n","NV3450\nDiscontinued\n","NV3458\nDiscontinued\n","NV5305\nDiscontinued\n","TA900\n1st Gen\nDiscontinued\n","TA900\n2nd Gen\nDiscontinued\n","TA900e \n1st Gen\nDiscontinued\n","TA900e \n2nd Gen\nDiscontinued\n","NV6240\nDiscontinued\n","NV6310\nDiscontinued\n","NV6355\nDiscontinued\n","NV6410\nDiscontinued\n","NV644\nDiscontinued\n","NV7060\nDiscontinued\n","NV7100\nDiscontinued\n"]
[null,"Part Number","170034xFx","17003148Fx","17004148Fx","1202890E1","1700630E1","17004660F1","17005660F1","42139xxFx","42439xxFx","470025xFx","4700633xG1","4700636xF1","1200520E1","4200510L1","1700515E2","1700601G2","1700611G2","1202860E1","1203860G1","1202870E1","1203870G1","1202880E1","1200820E1","1202820G1","1200821E1","1200823G1","1200824G1","4200990L1","42109xxL1","42129xxL1","42409xxL1","42429xxL1","474020xGxx","1700100G1","1200740E1","17006410F1","1700144G1","1700706G1","1200796E1"]
[null,"Firmware: Initial Release","11.04.1","R13.8.0","R13.8.0","07.01.00","17.04.02","R10.10.0","11.04.00","R13.9.0.HB","R10.09.00","R10.09.00","A3.03","R11.2.0","06.03.00","06.03.00","14.02.00","13.02.00","13.02.00","05.02.00 GT","17.02.02","05.02.00 GT","17.02.02","05.02.00","13.02.00","17.05.01","13.02.00","17.06.01","17.06.01","06.02.00","12.06.00","14.07.00","12.06.00","14.07.00","A5.01","A2.01","14.06.00","R11.3.0","A5.01","A1.03.00","15.09.00.SA"]
[null,"Firmware: Maintenance Release","R14.1.2","R14.1.2","R14.1.2","R14.1.2","R14.1.2","R14.1.2","R14.1.2","R14.1.2","R14.1.2","R14.1.2","R14.1.2","R14.1.2",null,null,"R13.2.3","R12.3.4","R12.3.4",null,"R14.1.2",null,"R14.1.2","R14.1.2","R14.1.2","R14.1.2","R14.1.2","R14.1.2","R14.1.2","R13.2.3","A4.10.00","R14.1.2","A4.10.00","R14.1.2","R13.2.3","R14.1.2","R13.2.3","R13.2.3","R13.2.3","R11.10.7 HA","R11.10.7 HA"]
[null,"Firmware: Feature Release","R14.1.0","R14.1.0","R14.1.0","R14.1.0","R14.1.0","R14.1.0","R14.1.0","R14.1.0","R14.1.0","R14.1.0","R14.1.0","R14.1.0","13.15.00","13.15.00","R13.4.0","R12.3.4","R12.3.4","15.12.00 GT","R14.1.0","15.12.00 GT","R14.1.0","R14.1.0","R13.10.0","R14.1.0","R14.1.0","R14.1.0","R14.1.0","R13.4.0","A4.11.00","R14.1.0","A4.11.00","R14.1.0","R13.4.0","R14.1.0","R13.4.0","R13.4.0","R13.4.0","R11.10.7 HA","R11.10.7 HA"]
[null,"Admin / Mgmt"]
[null,"Auto Configuration {AOS 11.01}","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","•","•","•","•","•","•","•","•","—","•","—","—","•","•","•","—","—","•","•"]
[null,"Bad Splice Detection EFM NIM2 {A4.05.00}","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—"]
[null,"Battery Status Monitor {R11.10.0}","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Cable Diagnostics {AOS 17.01.01}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Change LED Status State {R11.6.0.SA}","—","—","—","—","—","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"CLI Privilege Level Access (7 Levels) {R10.11.0}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","•","•","—","—"]
[null,"CPU Load History {R11.03.0}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","—","•","•","•","•","•","—","•","—","•","•","•","•","•","•","•","•"]
[null,"Event History (Max Increased to 256KB) {R11.5.0}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","•","•","—","—"]
[null,"Desktop Auditing {AOS 17.08.01}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"DHCP Network Forensics {AOS 17.08.01}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Ethernet OAM CFM {AOS 17.04.01}",{"$f":"$U$17","v":"—"},{"$f":"$U$17","v":"—"},"—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Ethernet OAM Using Y.1731",{"$f":"$U$17","v":"—"},{"$f":"$U$17","v":"—"},"—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Factory Reset CLI {AOS R13.8.0}","—","—","—","—","—","—","—","—","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Factory Reset SNMP {AOS R13.8.0}","—","—","—","—","—","—","—","—","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Flash Provisioning {AOS 17.01.01}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"FTP Server","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Generic Email Client {AOS 17.02.01}","•","•","•","•","•","•","•","—","—","—","—","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—"]
[null,"HTTP Web Configuration {AOS 5.01}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","—","—","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•"]
[null,"LLDP {AOS 8.01.00}","•","•","•","—","—","•","•","—","—","—","—","•","—","—","•","•","•","—","—","—","—","—","—","—","•","—","•","—","—","—","—","—","—","—","•","—","—","•","•"]
[null,"LLDP Inventory TLV {R11.5.0}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","•","•","—","—"]
[null,"LLDP Ignore Speed Mismatch {R10.11.0}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","—","—","—","—","—","—","—","•","—","•","—","—","—","—","—","—","—","•","—","—","—","—"]
[null,"LLDP-MED {AOS 17.02.01/A4.01.00}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","—","—","—","—","—","—","—","•","—","•","—","—","—","—","—","—","—","•","—","—","•Ŧ","•Ŧ"]
[null,"nCommand MSP Auto Link","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Network Quality Monitoring {AOS 17.02.01/A4.01.00}","•","•","•","•","•","•","•","•","•","•","—","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•"]
[null,"NetFlow 9 Export {AOS 17.02.01}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","•","•","•","•","—","•","•","•","•","—","•"]
[null,"Network Time Protocol {AOS 17.02.01/A4.01.00}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","—","IPv4/IPv6","—","—","•","•","•","—","•","—","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","—","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•Ŧ","•Ŧ"]
[null,"Packet Capture (Generic and SIP)  {AOS R10.1}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•",null,null,"—","•","—","•","—","•","•","•","•","•","•",null,"•",null,"•","—","•","•","•","•","•","•"]
[null,"Ping -- Set TOS/DSCP and DF Flag {R10.10.0}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","•","•","—","—"]
[null,"Portal Lists {AOS 17.01.01/A1.01.00}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"ProServices GUI {R11.4.1}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Restricted Boot Functionality {R11.4.0}","Boot Version\nR11.5.0","Boot Version\nR11.3.0.B2","Boot Version\nR11.3.0.B2","—","—","Boot Version\nR10.10.0.B5","Boot Version\nR11.4.1.B2","—","Boot Version\nR10.9.3.B2 ","Boot Version\nR10.9.3.B2 ","—","Boot Version\nR11.2.0.B1 ","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Safe Mode Download/RAM Disk {AOS 17.07.01}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"SCP Client (Secure Copy) {R10.10.0}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","•","•","—","—"]
[null,"SCP Public Key Authentication (Secure Copy) {R10.10.0}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","•","•","—","—"]
[null,"SFP Diagnostics {AOS 17.07.01}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"SNMP V1, V2c","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•"]
[null,"SNMP V3 {AOS 13.01} ","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•"]
[null,"SNMP Dying Gasp {R11.6.0.SA}","—","—","—","—","—","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"SNMP SFP Diagnostics {R13.2.0}","•","•","•","•","•","•","•","—","•","•","—","•","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—"]
[null,"SNMP FQDN as SNMP Trap Target {R13.2.0}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","—","—","—","•","—","•","•","—","•","•","•","•","•","—","•","—","•","•","•","•","•","•","—","—"]
[null,"SNMP User Login & Logout Traps {R13.2.0}","—","—","—","—","—",null,null,"—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"SNMP VDSL Status & Performance  Monitoring Stats {R13.2.0}","—","—","—","—","—",null,null,"—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"SNMP MEF Performance Stats {R13.2.0}","—","—","—","—","—",null,null,"—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"SNMP Trap Buffering {R13.3.0}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","—","—","—","•","—","•","•","—","•","•","•","•","•","—","•","—","•","•","•","•","•","•","—","—"]
[null,"Software Licensing in AOS {R11.8.0}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","•","•","—","—"]
[null,"SSH CLI {AOS 5.01}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•"]
[null,"SSH CLI 2048 bit Keys {R10.11.0}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","•","•","—","—"]
[null,"SSH CLI Public Key Authentication {R10.10.0}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","•","•","—","—"]
[null,"SSH Tunnel to Linux Server for Remote Access {R11.4.1}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"SSL (HTTPS) Web Configuration {AOS 6.01}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","—","—","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•"]
[null,"SSLv3 / TLS 1.0 (HTTPS) Web Configuration {AOS 15.01}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","—","—","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","•","•","•","—","•","—","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•"]
[null,"Switchport Scheduler {AOS 17.05/A4.01.00}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","•Ŧ","•Ŧ"]
[null,"SYSLOG","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"TCL Scripts {AOS 16.01.01}","•","•","•","•","•","•","•","—","—","—","—","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Telnet CLI","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•"]
[null,"Temperature Protection Feature {R11.6.0.SA}","—","—","—","—","—","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"TFTP Server {AOS 8.01}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•"]
[null,"Top Talker (Integrated Traffic Monitoring) \n{AOS 17.01.01/A1.02.00}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","•"]
[null,"Top Websites Reporting {AOS 16.01.01/A1.01.00}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","•","•","•","•","—","•","•","•","•","—","•"]
[null,"Tscan Support EFM NIM2 {A4.05.00}","—","—","—","—","—","—","—","—","—","—","•","—","—","—","•","—","—","—","—","—","—","—","—","—","•","—","•","—","—","—","—","—","—","•","—","—","—","—","—"]
[null,"Voice Quality Monitoring (VQM) {AOS 17.01.01 / A1.01.00}","Ŧ ","Ŧ ","Ŧ ","Ŧ ","Ŧ ","•","•","•","•","•","•","•","—","—","•","•","•","—","Ŧ ","—","Ŧ ","—","•","Ŧ ","Ŧ ","Ŧ ","Ŧ ","Ŧ ","•","•","•","•","•","•","•","•","•","—","•"]
[null,"VoIP Auto Configuration {R11.03.0}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"VoIP On Demand Report {R11.03.0}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"WLAN Automatic Security\nKey Generation {AOS 17.02.01}","•","•","•","•","•","•","•","—","—","—","—","•","—","—","•","•","•","—","•","—","•","—","•","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—"]
[null,"WLAN Controller NetVanta 150\n{AOS 15.01/A1.01.00}","24 APs","—","—","24 APs","24 APs","—","—","8 APs","8 APs","8 APs","8 APs","—","—","—","24 APs","8 APs","8 APs","—","8 APs","—","8 APs","—","24 APs","24 APs","24 APs","24 APs","24 APs","24 APs","8 APs","8 APs","8 APs","8 APs","24 APs","8 APs","8 APs","—","—","—","8 APs"]
[null,"WLAN Controller NetVanta 160\n{R10.4.0/R11.6.0.SA}","24 APs","—","—","24 APs","24 APs","24 APs\n{R11.6.0.SA}","24 APs\n{R11.6.0.SA}","8 APs","8 APs","8 APs","8 APs","24 APs\n{R11.6.0.SA}","—","—","24 APs","8 APs","8 APs","—","8 APs","—","8 APs","—","24 APs","24 APs","24 APs","24 APs","24 APs","24 APs","—","8 APs","—","8 APs","24 APs","8 APs","8 APs","—","—","—","8 APs"]
[null,"IPv6 Features"]
[null,"Address Resolution {AOS 18.1.1/R10.1.0}","•","•","•","—","•","•","•","—","•","•","•","•","—","—","•","—","—","—","—","—","—","—","•","•","•","•","•","•","—","—","—","•","•","•","•","•","•","—","—"]
[null,"Default Address Selection (Source Only)\n{AOS 18.1.1/R10.1.0}","•","•","•","—","•","•","•","—","•","•","•","•","—","—","•","—","—","—","—","—","—","—","•","•","•","•","•","•","—","—","—","•","•","•","•","•","•","—","—"]
[null,"Duplicate Address Detection {AOS 18.1.1/R10.1.0}","•","•","•","—","•","•","•","—","•","•","•","•","—","—","•","—","—","—","—","—","—","—","•","•","•","•","•","•","—","—","—","•","•","•","•","•","•","—","—"]
[null,"Lifetime Default Route {R11.5.0}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","—","—","—","—"]
[null,"MTU Learned from Router Advertisements {R11.5.0}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","—","—","—","—"]
[null,"Multicast Listener Discovery (MLD) {R11.4.1}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","—","—","—","—"]
[null,"Named Prefixes {R10.9.0}","•","•","•","—","•","•","•","—","•","•","•","•","—","—","•","—","—","—","—","—","—","—","•","•","•","•","•","•","—","—","—","•","•","•","•","•","•","—","—"]
[null,"Neighbor Discovery {AOS 18.1.1/R10.1.0}","•","•","•","—","•","•","•","—","•","•","•","•","—","—","•","—","—","—","—","—","—","—","•","•","•","•","•","•","—","—","—","•","•","•","•","•","•","—","—"]
[null,"Neighbor Unreachability Detection\n{AOS 18.1.1/R10.1.0}","•","•","•","—","•","•","•","—","•","•","•","•","—","—","•","—","—","—","—","—","—","—","•","•","•","•","•","•","—","—","—","•","•","•","•","•","•","—","—"]
[null,"Router Advertisement {AOS 18.1.1/R10.1.0}","•","•","•","—","•","•","•","—","•","•","•","•","—","—","•","—","—","—","—","—","—","—","•","•","•","•","•","•","—","—","—","•","•","•","•","•","•","—","—"]
[null,"Stateless Auto Configure (SLAAC)\n{AOS 18.1.1/R10.1.0}","•","•","•","—","•","•","•","—","•","•","•","•","—","—","•","—","—","—","—","—","—","—","•","•","•","•","•","•","—","—","—","•","•","•","•","•","•","—","—"]
[null,"Carrier Ethernet"]
[null,"Double-Tagged Y.1731 MEPs {R11.5.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Dynamic Packet Counters {R10.11.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Dynamic Queue Threshold Management {R13.3.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"EFM Bonding Auto-Detect  {R11.4.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Egress Shaping {R10.11.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"E-LMI in PE Mode {R11.5.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"E-LMI Status of Y.1731 MEPs & EFM Group Bandwidth {R11.6.0.SA}","—","—","—","—","—","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Enhanced Network Monitoring \nEFM Group Up/Down Speed {R10.11.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Enhanced Network Monitoring Interface Line Pool {R10.11.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Enhanced Network Monitoring \nY.1731 Loss of Continuity (LOC) {R10.11.0}","—","—","—","—","—","256 meps/mips","256 meps/mips","—","—","—","—","256 meps/mips","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Enhanced Network Monitoring \nY.1731 Remote Defect Indication (RDI) {R10.11.0}","—","—","—","—","—","256 meps/mips","256 meps/mips","—","—","—","—","256 meps/mips","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Enhanced Network Monitoring \nY.1731 Ability to poll MAC of Remote MEP {R13.3.0}","—","—","—","—","—","256 meps/mips","256 meps/mips","—","—","—","—","256 meps/mips","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Enhanced Network Monitoring \nY.1731 Ability to poll Defects for a Local MEP {R13.3.0}","—","—","—","—","—","256 meps/mips","256 meps/mips","—","—","—","—","256 meps/mips","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"EOC Dying Gasp {R11.6.0.SA}","—","—","—","—","—","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"E-TREE MEF {R11.5.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Forced Transmission of Y.1731 RDI's Based on Track {R11.5.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Globally Change EtherType {R11.6.0.SA}","—","—","—","—","—","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Hierarchical Policers {R11.5.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Hierarchical QOS w/Multiple Shapers to a Single Queue {R11.6.0.SA}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Ingress Policing/Limiting {R10.11.0}  UNI-to-MEN Direction Only, NOT from MEN-to-UNI.","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Jumbo Frame Support (up to 9200 bytes) {R11.6.0.SA}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Layer 2 Traffic Filter Based on MAC Address & EtherType {R11.5.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Layer 2 Transparent Mode {R10.11.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Max Number of EVC's {R11.5.0}","—","—","—","—","—",200,200,"—","—","—","—","200","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Max Number of EVC Maps","—","—","—","—","—",256,256,"—","—","—","—","256","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Max Number of Policers","—","—","—","—","—",1024,1024,"—","—","—","—","1024","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Multicast Address as Target MAC\nY.1731 Specify Class 1 Multicast Address as Target MAC {R11.10.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Per EVC Performance Monitoring Counters {R11.5.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Per Queue Shaping {R11.1.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Q-in-Q with pop and swap {R10.11.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Save Y.1731 Performance Monitoring Data (Per MEF 35) {R11.6.0.SA}","—","—","—","—","—","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Single Ended Y.1731 ETH-LM Functionality {R11.6.0.SA}","—","—","—","—","—","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"SPQ and WFQ QoS (8 Two-rate, 3 color CoS marking queues) {R10.11.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Synchronous Ethernet (Network Sync) Gigabit and SHDSL {R10.11.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"UNI/NNI failure notification {R10.11.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Unicast Frame Limiting {R11.6.0.SA}","—","—","—","—","—","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"VDSL Auto-Detect EFM Bonded & Non-Bonded Mode {R11.5.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"VDSL Retransmission Support G.993.8 {R11.5.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"VDSL Vectoring Support G.993.5 {R11.5.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"802.3ah Link OAM {R10.11.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Routing"]
[null,"ARP Cache Entries","1024 Per Int.","2577 Per Int. ","2577 Per Int. ","512 Per Int.","1024 Per Int.","1024 Per Int. (R12.3.0)","1024 Per Int. (R12.3.0)","256 Per Int.","1024 Per Int.","1024 Per Int.","256 Per Int.","1024 Per Int.","TBD","TBD","256 Per Int.","256 Per Int.","256 Per Int.","256 Per Int.","256 Per Int.","256 Per Int.","256 Per Int.","256 Per Int.","256 Per Int.","256 Per Int.","256 Per Int.","256 Per Int.","256 Per Int.","1024 Per Int.","256 Per Int.","256 Per Int.","256 Per Int.","256 Per Int.","256 Per Int.","256 Per Int.","256 Per Int.","2048 Per Int.","256 Per Int.","256 Per Int.","256 Per Int."]
[null,"ATM QoS (SHDSL NIM Only) {AOS 17.02.01}","•","•","•","•","•","—","—","—","—","—","—","—","—","—","•","—","—","—","•","—","•","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Backup Path Testing {18.01.01}","•","•","•","•","•","•","•","—","—","—","—","•","—","—","•","—","—","—","•","—","•","•","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"BGP in Multiple VRFs {AOS 18.03.01}","•","•","•","•","•","•","•","—","—","—","—","•","•","•","•","—","—","—","•","—","•","•","•","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—"]
[null,"BGP Route Redistribution to OSPF/RIP/Static {AOS 14.01}","•","•","•","•","•","•","•","•","•","•","—","•","—","—","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","—","—","—","—"]
[null,"Bridging {AOS 7.01}","•","•","•","•","•","•","•","—","—","—","—","•","•","•","•","—","—","•","•","•","•","•","•","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Demand Routing {AOS 11.01}","•","•","•","•","•","•","•","—","—","—","—","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—"]
[null,"DHCP","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","•"]
[null,"DHCP Client Option 60 {R10.10.0}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","•","•","—","—"]
[null,"DHCP Relay","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","•","IPv4/IPv6","—","—","—","•","•","—","•","—","•","•","—","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","•","—","•","•","•","•","•","—","—","—"]
[null,"DNS","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","•"]
[null,"DNS Proxy","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","•"]
[null,"Dynamic DNS {AOS 8.01}","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•"]
[null,"eBGP {AOS 8.01}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","—","IPv4/IPv6","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","—","—","—","—","—","• \n(2 Peers|300 Routes)"]
[null,"Enhanced Ethernet QoS {AOS 17.02.01}","20 shapers \nper QoS Map ","5 shapers \nper QoS Map ","5 shapers \nper QoS Map ","5 shapers \nper QoS Map","20 shapers \nper QoS Map Ŧ","• Ŧ","• Ŧ","5 shapers \nper QoS Map","TBD","TBD","—","• Ŧ","—","—","5 shapers \nper QoS Map","5 shapers \nper QoS Map","5 shapers \nper QoS Map","—","5 shapers \nper QoS Map","—","5 shapers \nper QoS Map","5 shapers \nper QoS Map","5 shapers \nper QoS Map","5 shapers \nper QoS Map","5 shapers \nper QoS Map","5 shapers \nper QoS Map","5 shapers \nper QoS Map","5 shapers \nper QoS Map","5 shapers \nper QoS Map","5 shapers \nper QoS Map","5 shapers \nper QoS Map","5 shapers \nper QoS Map","5 shapers \nper QoS Map","—","5 shapers \nper QoS Map","TBD","—","—","5 shapers \nper QoS Map"]
[null,"Enhanced Ethernet QoS for FR, PPP, HDLC, ATM\n{AOS 17.05.01/A4.01.00}","•","•","•","•","•","• Ŧ","• Ŧ","•","IPv4/IPv6","IPv4/IPv6","—","• Ŧ","—","—","•","•","•","—","•","—","•","•","•","•","IPv4/IPv6","•","IPv4/IPv6","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","•Ŧ"]
[null,"Fast Forwarding Engine FFE {AOS 13.01}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","•"]
[null,"Fast Forwarding Engine FFE Flow Bundling {R11.10.1}","—","—","—","—","—","IPv4/IPv6","IPv4/IPv6","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Rapid Route Service Assurance FFE {R11.10.0}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","—","•","•","•","•","—","—","—"]
[null,"Frame Relay","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","—","—","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","•"]
[null,"HDLC {AOS 9.01}","—","—","—","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","—","•"]
[null,"iBGP {AOS 10.01}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","—","IPv4/IPv6","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","—","—","—","—","—","• \n(2 Peers|300 Routes)"]
[null,"Integrated Route Bridging (IRB) {AOS 15.01}","—","—","—","T1-ETH Only","T1-ETH Only","—","—","—","—","—","—","—","—","—","T1-ETH Only","—","—","T1-ETH Only","T1-ETH Only","T1-ETH Only","T1-ETH Only","T1-ETH Only","T1-ETH Only","T1-ETH Only","T1-ETH Only","T1-ETH Only","T1-ETH Only","•","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Load Sharing {AOS 12.01}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","•"]
[null,"Multicast PIM Sparse Mode {AOS 11.01/A4.01.00}","•","•","•","•","•","•","•","•","•","•","—","•","—","—","•","—","—","—","—","—","—","•","•","•","•","•","•","•","•","•","•","•","•","—","•","—","—","—","•"]
[null,"Multicast Stub Routing {AOS 7.01/A4.01.00}","•","•","•","•","•","•","•","•","•","•","—","•","•","•","•","•","•","—","—","—","—","•","•","•","•","•","•","•","•","•","•","•","•","—","•","—","—","—","•"]
[null,"Multilink Frame Relay FRF16.1 {AOS 9.01}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","—","—","—","IPv4/IPv6","IPv4/IPv6","—","—","•","•","•","—","—","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","•","IPv4/IPv6","IPv4/IPv6","—","IPv4/IPv6","—","—","—","•"]
[null,"Multilink PPP (MLPPP) {AOS 7.01}","—","—","—","8 x T1","8 x T1","—","—","—","4 x T1","4 x T1","—","—","2 x T1","2 x T1","2 x T1","—","—","2 x T1","2 x T1","2 x T1","2 x T1","3 x T1","2 x T1","2 x T1","2 x T1","4 x T1","4 x T1","8 x T1","—","—","•","4 x T1","4 x T1","—","2 x T1","—","—","—","2 x T1"]
[null,"Multihoming {AOS 10.01}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","•","•","—","•","—","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","•"]
[null,"Network Monitor {AOS 13.01}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","—","—"]
[null,"OSPF v2 in Multiple VRFs {R11.03.0}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","—","•","•","—","•","—","•","—","—","•","•","•","•","•","—","•","—","•","•","•","•","—","—","—","•"]
[null,"OSPF v3","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","—","IPv4/IPv6","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","—","—","—","—","—","—"]
[null,"OSPF Distribute Lists {R11.4.1}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","—","—","—","—"]
[null,"OSPF Equal Cost Multipath {AOS 11.01}","•","•","•","•","•","•","•","•","•","•","—","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","—","—","—","—"]
[null,"Policy Based Routing {AOS 11.01}","•","•","•","•","•","•","•","•","•","•","—","•","—","—","•","—","—","—","•","—","•","•","•","•","•","•","•","•","•Ŧ","•","•","•","•","—","—","—","—","—","—"]
[null,"PPP †","•","•","•","•","•","—","—","•","•","•","—","—","•","•","•","—","—","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","•","—","—","—","•"]
[null,"PPP on Mef-Ethernet EFM NIM2 Module {R10.6.0}","—","—","—","—","—","—","—","—","—","—","IPv4/IPv6","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","IPv4/IPv6","—","—","—","—","•"]
[null,"PPPoA (W/ADSL NIM or ADSL Port) {AOS 8.01}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","—","—","—","—","—","IPv4/IPv6","—","•","•","•","—","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","—","—","IPv4/IPv6","IPv4/IPv6","—","—","—","•"]
[null,"PPPoE {AOS 5.01}","•","•","•","•","•","—","—","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","•"]
[null,"PPPoE on Ethernet Subinterfaces {R10.06.0}","•","•","•","•","•","—","—","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","—"]
[null,"PPPoFR (PPP and MLPPP over Frame Relay) {AOS 17.07.01}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","—","—","•","IPv4/IPv6","IPv4/IPv6","—","—","—","—","•","—","—","—","•","—","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","•","—","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","•"]
[null,"QoS Class Based\nWeighted Fair Queuing {AOS 10.1}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","•"]
[null,"QoS DiffServ Marking {AOS 6.01}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6 Ŧ","—","—","•"]
[null,"QoS FRF.12 Fragmentation {AOS 6.01}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","—","—","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","•","•","•","—","—","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","•"]
[null,"QoS Priority Queuing {AOS 6.01}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","•"]
[null,"QoS Rate Counters for Ingress & Egress {R11.4.1}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","•","•","•","—","•","—","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","•","—","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","—"]
[null,"QoS Weighted Fair Queuing {AOS 5.01}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","•"]
[null,"RIP v1/v2","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","—","•"]
[null,"Route Tags for Routing Protocols {R11.4.1}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","—","—","—","•","—","•","•","•","•","•","•","•","•","•","•","—","•","•","•","•","—","—","—","—"]
[null,"Strict Rate Policing {AOS 18.01.01}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","—","IPv4/IPv6","—","—","•","—","—","—","—","—","—","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Syslog in Non-Default VRF {R11.4.1}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","—","—","—","—"]
[null,"Traffic Shaping-Routed Interface {AOS 10.01}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","•"]
[null,"UDP Relay in Non-Default VRF {R10.10.0}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","—","—","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","—","—","—","—"]
[null,"VRF {AOS 16.01.01/A1.01.00}","8 VRF's\nIPv4/IPv6","8 VRF's\nIPv4/IPv6","8 VRF's\nIPv4/IPv6","8 VRF's","8 VRF's\nIPv4/IPv6","8 VRF's\nIPv4/IPv6","8 VRF's\nIPv4/IPv6","8 VRF's","8 VRF's\nIPv4/IPv6","8 VRF's\nIPv4/IPv6","8 VRF's\nIPv4/IPv6","8 VRF's\nIPv4/IPv6","—","—","•","—","—","—","8 VRF's","—","8 VRF's","8 VRF's","8 VRF's\nIPv4/IPv6","8 VRF's\nIPv4/IPv6","8 VRF's\nIPv4/IPv6","8 VRF's\nIPv4/IPv6","8 VRF's\nIPv4/IPv6","8 VRF's\nIPv4/IPv6","8 VRF's","8 VRF's","8 VRF's","8 VRF's\nIPv4/IPv6","8 VRF's\nIPv4/IPv6","8 VRF's\nIPv4/IPv6","8 VRF's\nIPv4/IPv6","—","—","—","—"]
[null,"VRF Firewall Option for Local Traffic Only {R11.4.1}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","•","—","—","—","IPv4/IPv6","—","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","IPv4/IPv6","—","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","—"]
[null,"VRRP {AOS 16.01.01/A4.01.00}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","•","•","•","—","•","—","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","•Ŧ"]
[null,"VRRP for VoIP {R12.2.0.SA}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","•","—","—","—"]
[null,"VxLAN Tunnels (VTEP) {R13.1.0}","•","•","•","—","•","•","•","—","—","•","—","•","—","—","—","—","—","—","—","—","—","—","—","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Switching"]
[null,"ActivChassis (Stacking) {AOS 10.7}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"ActivReach {R10.5.0}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Clustering (Single IP Address Management) {AOS 8.01}","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","—","—","—","—","—","—","—","—","—","•","—","•","—","—","—","—","—","—","—","•","—","—","•","•"]
[null,"CoS (802.1p) {AOS 5.01}","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","•","—","•","—","—","—","—","—","—","—","•","—","—","•","•"]
[null,"DiffServ to COS Mapping  {AOS 7.01}","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","•","—","•","—","—","—","—","—","—","—","•","—","—","•","•"]
[null,"Flow Control 802.3x {AOS 18.02.01}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"GVRP {AOS 8.01}","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","•","—","•","—","—","—","—","—","—","—","•","—","—","•","•"]
[null,"Guest Default VLAN for Non-802.1x Devices {R11.6.0.SA}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Hardware ACLs {AOS  17.03.01}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"IGMP Snooping {AOS 12.01}","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"IGMP Snooping Immediate Leave {R11.5.0}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"IGMP Querier {AOS R10.10)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","TBD","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"IGMP Subscribers ","—","—","—","—","—","—","—","—","—","—","—","—","—","—","TBD","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"IGMP Groups (Channels)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","TBD","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Jumbo Frames (MTU) {AOS  17.03.01}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Layer 3 Switching","—","—","—","—","—","—","—","—","—","—","—","—","—","—","L3 Lite","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Layer 3 Switching Interfaces","—","—","—","—","—","—","—","—","—","—","—","—","—","—",32,"—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Layer 3 Switching Routes","—","—","—","—","—","—","—","—","—","—","—","—","—","—",16,"—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Link Aggregation (802.3ad) {AOS 5.01}","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","•","—","•","—","—","—","—","—","—","—","•","—","—","•","•"]
[null,"MAC Table Entries","—","4K","4K","—","—","—","—","—","—","—","—","—","8K","8K","8K","4K","4K","—","—","—","—","—","—","—","4K","—","4K","—","—","—","—","—","—","—","8K","—","—","8K","8K"]
[null,"MAC Authentication Bypass {R11.5.0}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"PoE-802.3af {AOS 8.03}","—","17003148F11","17004148F11","—","—","—","—","—","—","—","—","—","4200570L1","4200530L1","1700525E2","—","—","—","—","—","—","—","—","—","4200821G11#120","—","4200824G11#120","—","—","—","—","—","—","—","•","—","—","•","•"]
[null,"PoE-802.3at {AOS 18.01.01}","—","17003148F11","17004148F11","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"PoE-Legacy {AOS 11.01}","—","17003148F11","17004148F11","—","—","—","—","—","—","—","—","—","—","—","1700525E2","—","—","—","—","—","—","—","—","—","4200821G11#120","—","4200824G11#120","—","—","—","—","—","—","—","•","—","—","•","•"]
[null,"Port Authentication 802.1x Supplicant Mode {AOS 9.01}","•","•","•","•","•","•","•","—","—","—","—","•","—","—","—","•","•","•","•","•","•","•","•","•","—","•","—","•","—","—","—","—","—","—","•","—","—","•","•"]
[null,"Port Authentication 802.1x Authenticator Mode {AOS 10.01}","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","•","—","•","—","—","—","—","—","—","—","•","—","—","•","•"]
[null,"Port Authentication 802.1x on Trunk Ports & Voice VLAN Ports {R11.13.0}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Port Security (MAC Based) {AOS 8.01}","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","•","—","•","—","—","—","—","—","—","—","•","—","—","•","•"]
[null,"Port Mirroring {AOS 5.01}","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","•","—","•","—","—","—","—","—","—","—","•","—","—","•","•"]
[null,"Protected Ports (Private VLAN Edge) {AOS 10.01}","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","•","•"]
[null,"Rapid Spanning Tree {AOS 5.01}","•","•","•","•","•","•","•","—","—","—","—","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","—","—","—","—","•","—","—","•","•"]
[null,"Spanning Tree","•","•","•","•","•","•","•","—","—","—","—","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","—","—","—","—","•","—","—","•","•"]
[null,"Spanning Tree Root Guard {R11.5.0}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Storm Control (Enhanced) {R11.8.0}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Storm Control","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"VLAN Aware Port Security {AOS 17.09.01}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","•","—","•","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"VLAN Interface {AOS 5.01}","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","•","•"]
[null,"VLAN Support (802.1Q)","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","•","•"]
[null,"Windows Machine Authentication/Port Authentication {R11.13.0}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Firewall & VPN"]
[null,"AAA Authentication","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"AAA with TACACS+ {AOS 11.01}","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Denial of Service (DoS) Protection ","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","•","—","•"]
[null,"DiffServ Preservation During VPN Encryption {AOS 7.01}","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","—","•"]
[null,"DMVPN (Dynamic Mode VPN) {R11.7.0}","EFP Only","EFP Only","EFP Only","EFP Only","EFP/SBC Only","•","•","•","•","•","•","•","—","—","•","•","•","—","EFP Only","—","EFP Only","EFP Only","EFP Only","EFP/SBC Only","EFP/SBC Only","EFP Only","EFP Only","EFP Only","—","•","—","•","•","•","•","—","—","—","•"]
[null,"GRE {AOS 9.01}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","•"]
[null,"GRE Ingress/Egress Policers {R11.9.0}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","•","•","•","—","•","—","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","•","—","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","•"]
[null,"GRE Multipoint Tunnels {R11.9.0}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","•","•","•","—","•","—","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","•","—","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","•"]
[null,"IPSEC ","500 Tunnels","500 Tunnels","500 Tunnels","500 Tunnels","1000 Tunnels","1000 Tunnels","1000 Tunnels","50 Tunnels","100 Tunnels","1000 Tunnels","10 Tunnels","1000 Tunnels","100 Tunnels","100 Tunnels","100 Tunnels","5 Tunnels","5 Tunnels","5 Tunnels","5 Tunnels","5 Tunnels","5 Tunnels","100 Tunnels","100 Tunnels","100 Tunnels","100 Tunnels","500 Tunnels","500 Tunnels","2000 Tunnels","5 Tunnels","5 Tunnels","10 Tunnels","30 Tunnels Ŧ","10 Tunnels","10 Tunnels","10 Tunnels","—","—","—","5 Tunnels"]
[null,"IP Crypto W/FFE {AOS 17.06.01}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","—","—","—","—","—","—","•","•","•","•","•","•","•","—","•","—","•","•","•","•","—","—","—","•"]
[null,"Maximum Firewall Associations (based on default RAM)","200K","200K SBC","450K ","80K","80K\n200K SBC","200K","200K","—","200K","200K","30K","200K","—","—","30K","—","—","—","10K","—","10K","10K","30K","30K\n200K SBC 100","30K\n200K SBC 100","80K","80K","80K","—","—","—","—","30K","30K","30K","—","—","—","30K"]
[null,"NAT 1 to 1","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","—","•"]
[null,"NAT 1 to 1 Port-Translation {AOS 10.01}","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","—","•"]
[null,"NAT Many to 1","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","—","•"]
[null,"NAT Preserve Source Port {AOS 14.01}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","—","•"]
[null,"Security Audit {AOS 17.07.01}","•","•","•","•","•","•","•","—","—","—","—","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Security Dashboard {AOS 17.05.01}","•","•","•","•","•","•","•","—","—","—","—","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Stateful Firewall","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","•"]
[null,"Stateless Allow Processing {AOS 12.01}","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—","—","—","•"]
[null,"Static 1:1 NAT Pools {AOS 17.04.01}","•","•","•","•","•","•","•","—","—","—","—","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—"]
[null,"URL Filtering {16.01.01}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","—","—"]
[null,"VPN Dead Peer Detection {7.01}","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","—","•"]
[null,"VPN NAT Traversal {7.01}","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","—","•"]
[null,"VPN Reverse Route Injection {AOS 15.01}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","—","•"]
[null,"VPN Tunnel Connection Using DNS Names {AOS 16.01.01}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","—","•"]
[null,"VPN X.509 Certificates","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","—","•","•","•","•","•","—","•","—","—","•","•","•","—","—","—","•"]
[null,"VPN Diffie-Hellman DH Group 1-5","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","—","•","•","•","•","•","—","•","—","—","•","•","•","—","—","—","•"]
[null,"VPN Encryption DES, 3DES, AES-128, AES-192, and AES-256","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","—","•","•","•","•","•","—","•","—","—","•","•","•","—","—","—","•"]
[null,"Web Content Filtering with Websense® {AOS 12.01}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","—","—","—","•","—","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","—","•"]
[null,"Voice Features"]
[null,"2 B-Channel Transfer (2BCT) {A2.05.00}","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","—","•","—","—"]
[null,"3 Way Conferencing FXS Users (Local to the unit)  {A1.02.00}","—","—","—","—","—","—","—","3 seperate \n3-way Conf","3 seperate \n3-way Conf","3 seperate \n3-way Conf","3 seperate \n3-way Conf","3 seperate \n3-way Conf","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","3 seperate \n3-way Conf","—","3 seperate \n3-way Conf","5 seperate \n3-way Conf","3 seperate \n3-way Conf","Limited to 1\n3-way Conf","—","—","—","—"]
[null,"Analog Loop Voltage Holdover Timer {R11.10.0}","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","•","•","•","•","—","—","—","—"]
[null,"Auto-ERL (Echo Return Loss) on Analog FXO Interfaces {A2.05.00}","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","—","—","•","•"]
[null,"Caller ID Name Override (external calls) per user {A4.02.00}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•"]
[null,"Call Pickup Groups {A2.05.00}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•"]
[null,"Call Queueing {A4.02.00}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•"]
[null,"Dial Plan Named Timeout {A2.03.00}","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Distinctive Call Waiting {A2.04.00}","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","—","—","—","—"]
[null,"Directed Call Pickup {A2.05.00}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•"]
[null,"DNIS out FXS as DTMF {A2.04.00}","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","—","—","•","•"]
[null,"DNS Cache for Transparent Proxy Phones {A4.03.00}","—","—","—","—","—","—","—","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","—","•","—","—","—","—"]
[null,"DS0 Leveling for TDM Trunks {A2.04.00}","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","•","•","•","•","—","•","—","—"]
[null,"Emergency Caller ID Override (per user) {A4.01.00}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•"]
[null,"Enhanced ANI Substitution {A2.03.00}","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Enhanced E911 Support {A2.06}","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","—","•","•","—","—"]
[null,"Enhanced IP Phone Config with CSV Import {A2.06}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•"]
[null,"ETSI PRI Overlap Signaling {A2.05.00}","—","—","—","—","—","—","—","—","—","—","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","—","•","—","—"]
[null,"Find Me / Follow Me {A4.01.00}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•"]
[null,"FXS Busy Out Support {R10.1.0}","—","—","—","—","—","—","—","—","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","—","—","—","—"]
[null,"FXS Automatic Dial {R11.10.0}","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","•","•","•","•","—","—","—","—"]
[null,"Handset Paging Groups {A2.04.00}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","10 Page \nGroups","10 Page \nGroups"]
[null,"Hot Desking / Hoteling {R10.7.0}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•"]
[null,"Internal Music on Hold {A4.02.00}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•"]
[null,"International FXO Support - Australia, Ireland, UK, and Mexico {A4.05.00}","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","—","—","•","•"]
[null,"International FXS Impedance and Tones - Australia, Belgium, Ireland, UAE, UK, and Mexico {A4.05.00}","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","—","—","•","•"]
[null,"ISDN Redirecting Number {A4.03.00.SC}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•"]
[null,"Loop Back Accounts {A1.01.00}","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Message Waiting Indicator (MWI) - FSK (MDF, SDMF)","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","—","—","•","•"]
[null,"Message Waiting Indicator (MWI) - Neon/Voltage (LED Only)","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","•","•","•","•","—","—","—","—"]
[null,"Modem Pass-through Auto Call Waiting Disable {A2.04.00}","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","—","—","—","—"]
[null,"Monitor SIP Voice User Registration State w/Tracks {R11.10.0}","—","—","—","—","SBC Only","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","SBC Only","SBC Only","—","—","—","—","•","—","•","•","•","•","•","—","•","•"]
[null,"Multilingual support for Voicemail and\nDial-By-Name Directory {A4.02.00}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•"]
[null,"Multiple SIP Signaling Ports  {A4.01.00}","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Proxy User Templates {AOS 17.09.01 / A4.02.00}","—","—","—","—","—","—","—","•","•","•","•","•","—","—","•","—","—","—","—","—","—","—","—","—","•","—","•","—","•","•","•","•","•","•","•","•","—","—","—"]
[null,"Ring Group Call Waiting {A4.02.00}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•"]
[null,"Ring Group DSP Resource Assignment {A4.01.00}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•"]
[null,"RFC 4904 Trunk Group Identifier {A2.05.00}","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","•","•","—","—"]
[null,"RTCP Sender Report {R10.7.0}","—","—","—","—","—","—","—","—","•","•","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Shared Call Appearances {A2.04.00}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•"]
[null,"SIP Header Manipulation Rules (HMR) {R10.1}","SBC Only","SBC Only","SBC Only","—","SBC Only","SBC Only","SBC Only","—","SBC Only","SBC Only","SBC Only","SBC Only","—","—","—","—","—","—","—","—","—","—","—","SBC Only","SBC Only","—","—","—","—","—","—","SBC Only","SBC Only","SBC Only","SBC Only","•","—","•Ŧ","•Ŧ"]
[null,"SIP Diversion Header {A1.03}","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","•","•","•","•"]
[null,"SIP Diversion and P-Asserted-Identity\nHeader Enhancement {A4.01.00}","—","—","—","—","—","—","—","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","—","•","•","•","—","—"]
[null,"SIP Media Loop Back {A4.03.00.SB}","SBC Only","SBC Only","SBC Only","—","SBC Only","SBC Only","SBC Only","—","SBC Only","SBC Only","SBC Only","SBC Only","—","—","—","—","—","—","—","—","—","—","—","SBC Only","SBC Only","—","—","—","•","—","•","SBC Only","SBC Only","SBC Only","•","•","•","—","—"]
[null,"SIP Proxy with Aliases {A4.03.00.SB}","EFP Only","EFP Only","EFP Only","EFP Only","EFP/SBC Only","•","•","•","•","•","•","•","—","—","•","•","•","—","EFP Only","—","EFP Only","EFP Only","EFP Only","EFP Only","EFP Only","EFP Only","EFP Only","EFP Only","•","•","•","•","•","•","•","•","—","—","—"]
[null,"SIP Proxy BLF {A4.01.00}","—","—","—","—","—","—","—","50 BLF Users","TBD","TBD","50 BLF Users","TBD","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","4 BLF Users","50 BLF Users","4 BLF Users","50 BLF Users","50 BLF Users","50 BLF Users","50 BLF Users","TBD","—","—","—"]
[null,"SIP Proxy Failover to PSTN","EFP/SBC Only Ŧ","EFP/SBC Only Ŧ","EFP/SBC Only Ŧ","EFP Only Ŧ","EFP/SBC Only Ŧ","•","•","•Ŧ","•Ŧ","•Ŧ","•","•Ŧ","—","—","•Ŧ","•Ŧ","•Ŧ","—","EFP/SBC Only Ŧ","—","EFP/SBC Only Ŧ","EFP/SBC Only Ŧ","EFP Only Ŧ","EFP/SBC Only Ŧ","EFP/SBC Only Ŧ","EFP/SBC Only Ŧ","EFP/SBC Only Ŧ","EFP Only Ŧ","•Ŧ","•Ŧ","•","•","•","•Ŧ","•","•Ŧ","—","—","—"]
[null,"SIP Proxy Shared Line Appearance {A2.04.00}","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","•","—","—","—"]
[null,"SIP Proxy Monitor (Stateful Proxy Mode)  {R10.9.0}","EFP/SBC Only","EFP/SBC Only","EFP/SBC Only","EFP Only","EFP/SBC Only","•","•","•","•","•","•","•","—","—","•","•","•","—","EFP/SBC Only","—","EFP/SBC Only","EFP/SBC Only","EFP Only","EFP/SBC Only","EFP/SBC Only","EFP/SBC Only","EFP/SBC Only","EFP Only","•","•","•","•","•","•","•","•","—","—","—"]
[null,"SIP Proxy Monitor (Transparent Proxy Mode)  {R11.9.0}","EFP/SBC Only","EFP/SBC Only","EFP/SBC Only","EFP Only","EFP/SBC Only","•","•","•","•","•","•","•","—","—","•","•","•","—","EFP/SBC Only","—","EFP/SBC Only","EFP/SBC Only","—","EFP/SBC Only","EFP/SBC Only","EFP/SBC Only","EFP/SBC Only","EFP Only","—","•","—","•","•","•","•","•","—","—","—"]
[null,"SIP Proxy Remote Survivability {AOS 17.03.01/Voice 16.03}","EFP/SBC Only","EFP/SBC Only","EFP/SBC Only","EFP Only","EFP/SBC Only","•","•","•","•","•","•","•","—","—","•","•","•","—","EFP/SBC Only","—","EFP/SBC Only","EFP/SBC Only","EFP Only","EFP/SBC Only","EFP/SBC Only","EFP/SBC Only","EFP/SBC Only","EFP Only","•","•","•","•","•","•","•","•","—","—","—"]
[null,"SIP Proxy Registration Rate Pacing {R11.6.0.SA}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","•","—","—","—"]
[null,"SIP Proxy Forking w/SCA {R11.6.0.SA}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","•","—","—","—"]
[null,"SIP Timers D & J {R10.10.0}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","•","—","—","—"]
[null,"SIP TLS and SRTP (SIP-to-SIP Trunks) {R13.2.1}","SBC Only","SBC Only","SBC Only","—","—","—","—","—","SBC Only","SBC Only","SBC Only","—","—","—","—","—","—","—","—","—","—","—","—","SBC Only","SBC Only","—","—","—","—","—","—","—","—","SBC Only","—","—","—","—","—"]
[null,"SIP TLS and SRTP (SIP-to-TDM) {R11.5.0}","—","—","—","—","—","—","—","—","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—"]
[null,"SIP TLS and SRTP (Stateful SIP Proxy Only) {R13.1.0}","SBC Only","SBC Only","SBC Only","—","—","—","—","—","SBC FP Required","SBC FP Required","—","—","—","—","—","—","—","—","—","—","—","—","—","SBC Only","SBC Only","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"SIP Transparent Proxy {AOS 17.03.01/Voice 16.03}","•","•","•","•","•","—","—","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—","—"]
[null,"SIP Transparent Proxy Caching DNS {A4.03.00.SB}","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","•","—","—","—"]
[null,"SIP Subscribe Request Support for MWI {R10.10.0}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","•","—","—","—"]
[null,"SIP Server Monitor Recovery Delay {R11.6.0.SA}","•","•","•","•","•","•","•","•","•","•","•","•","—","—","•","•","•","—","•","—","•","•","•","•","•","•","•","•","—","•","—","•","•","•","•","•","—","—","—"]
[null,"Source and ANI Based Routing (SABR) {A2.03.00}","—","—","—","—","SBC Only","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","SBC Only","SBC Only","—","—","—","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Status Groups configurable \"notify ringing\" {A2.07}","—","—","—","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","•","•","•","•","—","•","—","•","—","—","—","—","—","—","—","—","—","•","•"]
[null,"Voicemail Class of Service defined as default {A2.07}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•"]
[null,"Voicemail WAV Attachment to Email {A2.01.00}","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•"]
[null,"Call Control"]
[null,"SIP","SBC Only","SBC Only","SBC Only","—","SBC Only","—","—","•","IPv4/IPv6","IPv4/IPv6","•","IPv4/IPv6","—","—","—","—","—","—","—","—","—","—","—","SBC Only","SBC Only","—","—","—","•","•","•","•","•","•","•","•","•","•","•"]
[null,"MGCP {A1.02.00}","—","—","—","—","—","—","—","FXS LS/GS","FXS LS/GS","FXS LS/GS","FXS LS/GS","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","FXS LS/GS","—","FXS LS/GS","FXS LS/GS","FXS LS/GS","—","—","—","—","—"]
[null,"CODECs"]
[null,"G.711","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","—","•","•","•"]
[null,"G.722","—","—","—","—","—","—","—","Ŧ","Ŧ","Ŧ","Ŧ","Ŧ","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","Ŧ","Ŧ","Ŧ","Ŧ","Ŧ","Ŧ","Ŧ","Ŧ","Ŧ","•","•"]
[null,"G.729a","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","—","•","•","•"]
[null,"Echo-tail Length","—","—","—","—","—","—","—","64 ms","64 ms","64 ms","64 ms","64 ms","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","16 ms","64 ms","16 ms","64 ms","64 ms","64 ms","64 ms","—","128ms","64 ms","64 ms"]
[null,"SBC Upgrade Features"]
[null,"SBC Licensable {R11.8.0}","•","•","•","—","—","•","•","—","•","•","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"SBC Feature Pack Fixed Capacity Upgrade {R10.1}","—","—","—","—","•","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","•","•","—","—","—","—","—","—","•","•","•","•","•","—","—","—"]
[null,"Codec Transcoding G.711 to G.729 {R10.4}","—","—","—","—","—","—","—","—","30","36","15","36","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","30","30","15","15","—","—","•","•"]
[null,"DTMF Tone Conversion In-Band to Out-of-Band {R10.4}","—","—","—","—","—","—","—","—","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","—","—","—","—"]
[null,"Media Anchoring {R10.1}","SBC Only","SBC Only","SBC Only","—","SBC Only","SBC Only","SBC Only","—","SBC Only","SBC Only","SBC Only","SBC Only","—","—","—","—","—","—","—","—","—","—","—","SBC Only","SBC Only","—","—","—","—","—","—","SBC Only","SBC Only","SBC Only","SBC Only","•","—","—","• FmFm Only"]
[null,"Remote Phone/SIP Support (Far-end NAT Traversal) {R10.1}","SBC Only","SBC Only","SBC Only","—","SBC Only","SBC Only","SBC Only","—","SBC Only","SBC Only","SBC Only","SBC Only","—","—","—","—","—","—","—","—","—","—","—","SBC Only","SBC Only","—","—","—","—","—","—","SBC Only","SBC Only","SBC Only","SBC Only","•","—","—","•"]
[null,"SIP Failover to PSTN","—","—","—","—","—","—","—","—","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—"]
[null,"SIP Normalization {R10.1}","SBC Only","SBC Only","SBC Only","—","SBC Only","SBC Only","SBC Only","—","SBC Only","SBC Only","SBC Only","SBC Only","—","—","—","—","—","—","—","—","—","—","—","SBC Only","SBC Only","—","—","—","—","—","—","SBC Only","SBC Only","SBC Only","SBC Only","•","—","—","—"]
[null,"Topology/Address Hiding ","SBC Only","SBC Only","SBC Only","—","SBC Only","SBC Only","SBC Only","—","SBC Only","SBC Only","SBC Only","SBC Only","—","—","—","—","—","—","—","—","—","—","—","SBC Only","SBC Only","—","—","—","—","—","—","SBC Only","SBC Only","SBC Only","SBC Only","•","—","—","—"]
[null,"Voice Interfaces"]
[null,"Emulation (Network Role)"]
[null,"FXS Loop Start","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","—","—","•","•"]
[null,"FXS Ground Start ","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","—","—","•","•"]
[null,"FXO DPT ","—","—","—","—","—","—","—","•","•Ŧ","•Ŧ","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•Ŧ","•Ŧ","•","•","•","—","—","—","—"]
[null,"ISDN PRI","—","—","—","—","—","—","—","•","•","•","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","—","•","—","•"]
[null,"T1 CAS E&M Wink","—","—","—","—","—","—","—","•","•","•","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","—","•","—","—"]
[null,"T1 CAS E&M Immediate","—","—","—","—","—","—","—","•","•","•","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","—","•","—","—"]
[null,"T1 CAS Loop Start","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"T1 CAS Ground Start","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"T1 CAS Feature Group D","—","—","—","—","—","—","—","•","•","•","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","—","•","—","—"]
[null,"Termination (User Role)"]
[null,"FXO Full Time PSTN","—","—","—","—","—","—","—","—","•Ŧ","•Ŧ","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","—","—","•","•"]
[null,"FXO Loop Start","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","•","•","•","—","—","•","•"]
[null,"FXO Ground Start","—","—","—","—","—","—","—","•","•Ŧ","•Ŧ","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•Ŧ","•Ŧ","•","•","•","—","—","•","•"]
[null,"ISDN PRI","—","—","—","—","—","—","—","—","•","•","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•","—","•","•","•"]
[null,"T1 CAS E&M Wink","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•"]
[null,"T1 CAS E&M Immediate","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•"]
[null,"T1 CAS Loop Start","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•"]
[null,"T1 CAS Ground Start","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•"]
[null,"T1 CAS Feature Group D","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•"]
[null,"Performance"]
[null,"Aggregate Routing Performance - (Eth-to-Eth)"]
[null,"Routing  - FW & NAT Throughput (IMIX Traffic)","600 Mbps","1 Gbps","2 Gbps @64byte","125 Mbps","700 Mbps","700 Mbps","2 Gbps","TBD","180 Mbps","200 Mbps","50 Mbps","700 Mbps","30 Mbps","30 Mbps","75 Mbps","25 Mbps","25 Mbps","—","—","—","—","60 Mbps","100 Mbps","100 Mbps","100 Mbps","150 Mbps","150 Mbps","150 Mbps","—","—","—","50 Mbps","TBD","50 Mbps","90 Mbps","—","—","—","30 Mbps"]
[null,"Routing - FW/NAT with QOS & Shaping Throughput (IMIX Traffic) ","150 Mbps","TBD","2 Gbps @64byte","90 Mbps","150 Mbps","150 Mbps","2 Gbps","TBD","100 Mbps","175 Mbps","25 Mbps","150 Mbps","15 Mbps ","15 Mbps","20 Mbps","10 Mbps","10 Mbps","—","—","—","—","30 Mbps","50 Mbps","50 Mbps","50 Mbps","100 Mbps","100 Mbps","100 Mbps","—","—","—","50 Mbps","TBD","25 Mbps","35 Mbps","—","—","—","20 Mbps"]
[null,"Routing - VPN Throughput (IMIX Traffic)","100 Mbps","200 Mbps","400 Mbps (EFP)","25 Mbps (EFP)","60 Mbps (EFP)","70 Mbps","70 Mbps","TBD","40 Mbps","60 Mbps","8 Mbps","70 Mbps","5 Mbps (EFP)","5 Mbps (EFP)","15 Mbps","1 Mbps","1 Mbps","—","—","—","—","20 Mbps (EFP)","30 Mbps (EFP)","30 Mbps (EFP)","30 Mbps (EFP)","50 Mbps (EFP)","50 Mbps (EFP)","60 Mbps (EFP)","—","—","—","8 Mbps","TBD","8 Mbps","6 Mbps","—","—","—","5 Mbps"]
[null,"Voice Performance"]
[null,"Max Simultaneous TDM to IP Call Conversions","—","—","—","—","—","—","—",30,"60","72",30,"72","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—",24,30,48,60,60,30,"30","—",120,24,24]
[null,"Max Number of Calls on a Single Trunk (Non-SBC)","—","—","—","—","—","—","—",42,"100","200",84,"200","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—",42,42,84,"100",84,84,84,"1000","—",100,100]
[null,"Max T.38 Sessions (Version 0, 14.4 kbps)","—","—","—","—","—","—","—","30","30","60",4,"60","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—",1,4,1,4,"—",4,4,"TBD",120,2,2]
[null,"Max Number of Configured SIP Trunks","20-SBC Only","5-SBC Only","25 - SBC Only","—","5 -SBC Only","5 -SBC Only","5 -SBC Only","3","12","12","12","12","—","—","—","—","—","—","—","—","—","—","—","5 -SBC Only","5 -SBC Only","—","—","—",3,"3",3,"12","12","12","12","5","12",10,10]
[null,"SIP SBC -  Max Simultaneous Calls B2BUA (100% VQM & Media Anchoring)","300-SBC Only","300-SBC Only","1000-SBC Only","—","300 - SBC Only","300 - SBC Only","300 - SBC Only","—","100 - SBC Only","200 - SBC Only","50 - SBC Only","200 - SBC Only","—","—","—","—","—","—","—","—","—","—","—","50 - SBC50\n100 - SBC100","40 - SBC40\n100 - SBC100","—","—","—","—","—","—","50 -SBC Only","50 - SBC Only","50 - SBC Only","50 - SBC Only","1000","—","—","—"]
[null,"SIP Proxy - Max Simultaneous Calls (0% VQM)","TBD","TBD","TBD","TBD","450 - SBC Only","TBD","TBD","—","375","550","158","550","—","—","TBD","20","20","—","—","—","—","TBD","—","140 - EFP/SBC50\n250 - SBC100","140 - EFP/SBC40\n250 - SBC100","TBD","TBD","TBD","—","—","—","200","204","158","204","TBD","—","—","—"]
[null,"SIP Proxy - Max Simultaneous Calls (100% VQM)","TBD","TBD","TBD","TBD","300 - SBC Only","TBD","TBD","—","250","400","35","400","—","—","25","10","10","—","—","—","—","TBD","—","100 - EFP/SBC50\n120 - SBC100","100 - EFP/SBC40\n120 - SBC100","200 - EFP","200 - EFP","TBD","—","—","—","120","48","35","48","TBD","—","—","—"]
[null,"SIP Proxy - Maximum SIP Transaction Resources","3000","5000","10000\nŦ - AOS R13.9.0 ","TBD","3000 - SBC Only","3000","3000","—","1500","2000","500","2000","—","—","250","125","125","—","—","—","—","125 - EFP","—","300 - SBC50\n500 - EFP\n900 - SBC100","300 - SBC40\n500 - EFP\n900 - SBC100","500 - EFP","500 - EFP","TBD","—","—","—","600","500","500","500","10,000","—","—","—"]
[null,"Supported Modules"]
[null,"Dial-backup Interface Module (DIM)"]
[null,"Analog Modem DIM (1200864L1) Ŧ","—","—","—","•","•","—","—","—","—","—","—","—","•","•","•","—","—","•","•","•","•","•","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"ISDN BRI DIM (1200865L1) Ŧ","—","—","—","•","•","—","—","—","—","—","—","—","•","•","•","—","—","•","•","•","•","•","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Network Interface Module (NIM)"]
[null,"3G CDMA NIM (170080xG1) {AOS 17.02}","—","—","—","•","•","—","—","—","—","—","—","—","—","—","•","—","—","—","•","—","•","•","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"56/64K NIM (1200861L1)","—","—","—","•","•","—","—","—","—","—","—","—","•","•","•","—","—","•","•","•","•","•","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"ADSL NIM -- Annex A (1202869E1)","—","—","—","•","•","—","—","—","—","—","—","—","•","•","•","—","—","•","•","•","•","•","•","•","•","•","•","—","—","—","—","—","—","—","•","—","—","—","•"]
[null,"DIM Carrier Module (1200877L1)","—","—","—","•","•","—","—","—","—","—","—","—","•","•","•","—","—","•","•","•","•","•","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Dual T1 NIM (1200872L1)","—","—","—","•","•","—","—","—","—","—","—","—","•","•","•","—","—","•","•","•","•","Ŧ •","•","•","•","•","•","—","—","—","—","—","—","—","•","—","—","—","•"]
[null,"Dual T1 NIM (2nd Gen) {1202872L1} {AOS 17.09.01}","—","—","—","•","•","—","—","—","—","—","—","—","—","—","•","—","—","—","•","—","•","Ŧ •","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","•"]
[null,"Serial NIM (1200866E1)","—","—","—","•","•","—","—","—","—","—","—","—","•","•","•","—","—","•","•","•","•","•","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"SHDSL NIM -- Annex A (1200936E1)","—","—","—","•","•","—","—","—","—","—","—","—","•","•","•","—","—","•","•","•","•","•","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"T1/Fractional T1 NIM (1202862L1)","—","—","—","•","•","—","—","—","—","—","—","—","•","•","•","—","—","•","•","•","•","•","•","•","•","•","•","—","—","—","—","—","—","—","•","—","—","—","•"]
[null,"T1/Fractional T1 + DSX-1 NIM (1202863L1)","—","—","—","•","•","—","—","—","—","—","—","—","•","•","•","—","—","•","•","•","•","•","•","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"USB WWAN 2nd Gen (1702803F1)","—","—","—","—","•","—","—","—","—","—","—","—","•","•","—","—","—","—","—","—","—","•","—","•","•","•","•","—","—","—","—","—","—","—","—","—","—","—","•"]
[null,"Network Interface Module 2 (NIM2)"]
[null,"2W/4W SHDSL ATM NIM2 (1700101G1) ","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—"]
[null,"ADSL2+ NIM2 -- Annex A (1700114G1)","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—"]
[null,"Quad BRI S/T NIM2 (1700112G1)","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—"]
[null,"Quad SHDSL EFM NIM2 -- Annex A (1700103G1)","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—"]
[null,"Quad T1/E1 EFM NIM2 (1700106G1)","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—"]
[null,"Voice Interface Module (VIM)"]
[null,"Dual FXO/Dual FXS VIM (1202692G1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","•","•"]
[null,"Quad FXS (Station) VIM (1200690E1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","•","•"]
[null,"Quad FXO (Trunk) VIM (1202691G1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","•","•"]
[null,"T1/PRI VIM (1200695L1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","•","•"]
[null,"E1/PRI VIM (1200696G1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","•","•"]
[null,"Voice Interface Module 2 (VIM2)"]
[null,"Octal FXS VIM2 (1700108G1)","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—"]
[null,"Octal FXO VIM2 (1700109G1)","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—"]
[null,"Quad FXO/Quad FXS VIM2 (1700111G1)","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—"]
[null,"Quad FXO VIM2 (1700105G1)","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—"]
[null,"Quad FXS VIM2 (1700102G1)","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—"]
[null,"Wide Network Interface Module "]
[null,"HSSI Wide Module (1200934L1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Octal T1/E1 Wide Module (1202843E1)","—","—","—","•","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Unchannelized T3 Wide Module (1200832L1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","Ŧ •","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Carrier EFM (Ethernet First Mile) Modules"]
[null,"Quad VDSL2 EFM Module Annex A (17406369F1) {R11.2.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Quad VDSL2 EFM Module Annex B (17406369F3)  {R11.2.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Quad SHDSL EFM Module Annex A (17406368F1)  {R11.2.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Quad SHDSL EFM Module Annex B (17406368F3)  {R11.2.0}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Octal SHDSL EFM Module Annex A (17806368F1) {R11.2.1}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Octal SHDSL EFM Module Annex B (17806368F3){R11.2.1}","—","—","—","—","—","•","•","—","—","—","—","•","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Small Form-factor Pluggable Transceiver (SFP)"]
[null,"1000BaseLX -- 1310nm SFP (1200481E1)","—","—","—","—","•","•","•","—","—","•","—","•","•","—","•","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","•","—","—","•","•"]
[null,"1000BaseSX -- 850nm SFP (1200480E1)","—","—","—","—","•","•","•","—","—","•","—","•","•","—","•","—","—","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","—","—","•","—","—","•","•"]
[null,"Enhanced 2.5 Gbps Multimode SFP (1200482G1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Enhanced 2.5 Gbps Singlemode SFP (1200483G1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"1000BaseT Ethernet SFP (1200485G1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"10GBase-SR SFP+ Transceiver (1700485F1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"10GBase-LR SFP+ Transceiver (1700486F1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"1M Interconnect Cable SFP (1200484G1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—",null,"—",null,"—","—",null,"—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•"]
[null,"3M Interconnect Cable SFP (1200484G3)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—",null,"—",null,"—","—",null,"—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•"]
[null,"XIM Modules"]
[null,"Dual SFP XIM Module (1700473F1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Dual SFP+ XIM Module (1700471F1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Stacking XIM (1700470F1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Physical Specifications"]
[null,"Chassis Weight","1lb(DT) / 3lbs(RM)","3lbs","3lbs","7.5lbs","7.5lbs","7 lbs","7 lbs","5.5lbs 908\n7lbs 916/924","5.5lbs 908e\n7lbs 916e/924e","7lbs","7lbs","7 lbs","7lbs","7lbs","12lbs","1lb","1lb","2lbs","2lbs","7lbs","7lbs","7.5lbs","4lbs","4lbs","4lbs","7.5lbs","7.5lbs","21lbs","Ŧ 3.5lbs - 5.5lbs","Ŧ 3.5lbs - 5.5lbs","6.5lbs","6.5lbs","6.5lbs","7lbs","11lbs","7lbs","5.0lbs","11lbs","11lbs"]
[null,"Ethernet Interfaces (Physically Addressable)","3 - 10/100/1000","2 - 10/100/1000","2 - 10/100/1000","2 - 10/100","1 - 10/100","—","—","1 - 10/100/1000","2 - 10/100\n1 - 10/100/1000","4 - 10/100\n1 - 10/100/1000","2 - 10/100","4 - 10/100/1000","—","—","—","1 - 10/100","—","1 - 10/100","1 - 10/100","1 - 10/100","1 - 10/100","2 - 10/100","2 - 10/100","2 - 10/100","2 - 10/100","2 - 10/100","2 - 10/100","2 - 10/100","—","1 - 10/100","2 - 10/100","2 - 10/100","2 - 10/100","2 - 10/100","1 - 10/100","2 - 10/100/1000","2 - 10/100","—","1 - 10/100"]
[null,"Combo  Interfaces - Eth/SFP (Physically Addressable)","—","2 Combo","2 Combo","—","2 Combo","4 Combo","4 Combo","—","—","1 Combo","—","1 Combo","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—",null,"—","—","—","—","—","—","—","—","—"]
[null,"SFP Interfaces (Physically Addressable)","—","—",{"$f":"$AC$437","v":"—"},"—",{"$f":"$F$437","v":"—"},"1 - 1000BaseT","1 - 1000BaseT","—","—",{"$f":"$K$437","v":"—"},"—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Ethernet Switch Ports (Copper)","—","8 - 10/100/1000","8 - 10/100/1000","—","—","—","—","—","—","—","—","—","24 - 10/100\n1 - 10/100/1000","24 - 10/100","24 - 10/100\n2 - 10/100/1000","4 - 10/100","4 - 10/100","—","—","—","—","—","—","—","8 - 10/100","—","8 - 10/100","—","—","—","—","—","—","—","24 - 10/100\n2 - 10/100/1000","—","—","24 - 10/100\n2 - 10/100/1000","24 - 10/100\n2 - 10/100/1000"]
[null,"Ethernet Switch Ports (Fiber SFP Slots)","—","—","—","—","—","—","—","—","—","—",null,"—","1 Combo","—","2 Combo","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","2 Combo","—","—","2 Combo","2 Combo"]
[null,"Mean Time Between Failure (MTBF)","1,500,083 Hrs (DT)\n1,383,586 Hrs (RM)","1387136 Hrs.","1265039 Hrs.","923,225 Hrs","542,983 Hrs","516,601 Hrs","516,601 Hrs","850,247 Hrs","Ŧ 606,212 Hrs","Ŧ 448,401 Hrs","Ŧ 358,064 Hrs","TBD","700,717 Hrs","724,434 Hrs","224,193 Hrs","1,801,251 Hrs","1,705,670 Hrs","588,236 Hrs","1,604,107 Hrs","596,659 Hrs","1,445,442 Hrs","951,457 Hrs","349,896 Hrs","937,788 Hrs","686,686 Hrs","778,538 Hrs","664,435 Hrs","400,542Hrs","Ŧ 192,849 Hrs","Ŧ 314,108 Hrs","Ŧ 129,391 Hrs","Ŧ 305,388 Hrs","Ŧ 371,316, hrs","663,293 Hrs","264,251 Hrs","TBD","394,834 hrs","261,519 Hrs","261,519 Hrs"]
[null,"Operating Temperature (relative humidity up to 95% non-Condensing)","32°F to 122°F","32°F to 113°F","32°F to 113°F","32°F to 122°F","32°F to 122°F","-13°F to 158°F","-13°F to 158°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","TBD","32°F to 122°F","32°F to 122°F","32°F to 122°F"]
[null,"Rack Mount Dimensions","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","—","—","—","—","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","3U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\""]
[null,"RAM Size","512","1 GB","2 GB","256MB","256MB\n512MB (SBC)","512 MB","512 MB","64MB","512 MB","512 MB","128MB","512 MB","32MB","32MB","128MB","64MB","64MB","32MB","64MB","32MB","64MB","64MB","128MB","128MB\n512MB (SBC 100)","128MB\n512MB (SBC 100)","256MB","256MB","256MB","64MB","64MB","64MB","128MB","128MB\n512MB (optional)","128MB","128MB","TBD","128MB","128MB","128MB"]
[null,"RAM Upgrade Capacity","—","—","—","—","1024MB","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","512MB","512MB","512MB","512MB","512MB","1024MB","—","—","—","—","512MB ","—","—","—",null,"—","—"]
[null,"Flash Size","128MB","1 GB","1 GB","32MB","32MB","128 MB","128 MB","32MB","128 MB","256 MB","64MB","256 MB","16MB","16MB","32MB","32MB","32MB","16MB","32MB","16MB","32MB","16MB","32MB","32MB","32MB","32MB","32MB","32MB","16MB","32MB","32MB","32MB","128MB","64MB","32MB","TBD","64MB","32MB","32MB"]
[null,"T1 Interfaces (Built Into Chassis)","—","—","—","—","—","—","—","1-T1 + 1-DSX-1","4","4","—","2","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","1-T1 + 1-DSX-1","1-T1 + 1-DSX-1","4","4","4","1","—","—","4","—","—"]
[null,"Analog Interfaces (FXO)","—","—","—","—","—","—","—","8- Optional","1 - Optional\n9- Optional","1 - Optional\n9- Optional","16-Optional","1","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","8- Optional","8- Optional","1 - Built-in\n8 - Optional","1 - Built-in\n8 - Optional","2 - Optional\n10- Optional","16-Optional","2-Built-in\n10- Optional","—","—","2-Built-in\n10- Optional","2-Built-in\n10- Optional"]
[null,"Analog Interfaces (FXS)","—","—","—","—","—","—","—"," 8, 16, 24","8, 16, 24","8, 16, 24","32-Optional","8, 16, 24","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","4, 8, 12, 16, 24","4, 8, 12, 16, 24","8, 16, 24","8, 16, 24","8, 16, 24","16-Optional","2-Built-in\n10- Optional","—","—","2-Built-in\n10- Optional","2-Built-in\n10- Optional"]
[null,"USB Port(s)","—",1,1,"—","—","Ŧ ","Ŧ ","—","Ŧ ","Ŧ ","—","Ŧ ","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","Ŧ ","—","—","—"]
[null,"USB Port (LTE USB Modem Support)","VZ-Novatel 551L \nAT&T-Netgear 340U\nSprint-NetGear 341U ","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Internal Fan(s)","—","2","2","• 1x","• 2x","• 2x","• 2x","—","—","—","—","• 3x","TBD","TBD","• 1x \n• 3x (PoE)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","• 3x","—","• 1x","• 3x","• 3x"]
[null,"CompactFlash® Slot","—","—","—","—","•","—","—","—","—","—","•","—","—","—","•","—","—","—","—","—","—","—","•","•","•","•","•","—","—","—","—","—","—","•","•","—","—","•","•"]
[null,"Power Specifications"]
[null,"AC Power Supply","12VDC Adapter\n(Desk Version)\n100-250VAC\n(RM Verion)","100-250VAC","100-250VAC","100-250VAC","110-250VAC","110-250VAC","110-250VAC","120 VAC","120 VAC","120 VAC","100-240 VAC","110-240 VAC","100-250 VAC","100-250 VAC","120 VAC","12VDC (Adapter)","12VDC (Adapter)","12VDC (Adapter)","12VDC (Adapter)","100-250VAC","100-250VAC","100-250VAC","100-250VAC","100-250VAC","100-250 VAC","100-250VAC","100-250VAC","85–250 VAC","120 VAC","120 VAC","120 VAC","120 VAC","120VAC","100–240 VAC","100–250 VAC","100-240 VAC","100–240 VAC","100–250 VAC","100–250 VAC"]
[null,"DC Power Supply","12 VDC/1.0 A","—","—","-48 +24VDC","—","-48VDC/.8A","-48VDC/.8A","—","—","-48VDC/1.75A Max","—","-48VDC/1.5A Max",null,"—","—","—","—","—","—","-48 +24VDC","-48 +24VDC","—","—","—","—","—","—","-48 +24VDC","—","—","—","—","—","—","—","TBD","—","—","—"]
[null,"Max BTU",164,"TBD","TBD",258,258,"136","136",180,"255 908e\n374 916e/924e","374",103,"290",86,86,124,21,21,21,21,21,21,21,86,"85","85",21,21,1120,180,180,180,180,180,103,"—","TBD",180,"—","—"]
[null,"Max BTU with PoE Ŧ","—","TBD","TBD","—","—","—","—","—","—","—","—","—","1700","1700","1700","—","—","—","—","—","—","—","—","—",515,"—",450,"—","—","—","—","—","—","—",1550,"—","—",1550,1550]
[null,"Max Wattage  (Non-POE Models)","48W","TBD","TBD","75W","75W","40W","40W","75W 908\n110W 916/924","75W 908e\n110W 916e/924e","110W","30W","85W","25W","25W","36W","6W","6W","6W","6W","6W","6W","6W","25W","25W","25W","6W","6W","325W","53W","53W","53W","53W","53W","30W","—","TBD","50W","—","—"]
[null,"Max Wattage with PoE Ŧ","—","TBD","220W","—","—","—","—","—","—","—","—","—","500W","500W","500W","—","—","—","—","—","—","—","—","—","150W","—","130W","—","—","—","—","—","—","—","450W","—","—","450W","450W"]
[null,"PoE Power Budget","—","TBD","185W","—","—","—","—","—","—","—","—","—","370W","370W","370W","—","—","—","—","—","—","—","—","—","120W","—","120W","—","—","—","—","—","—","—","370W","—","—","370W","370W"]
[null,"EPS Support","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RPS Support","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]