{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["AOS Switch Feature Matrix"],"not_rendered":{"charts":0,"images":23,"macros":1,"external_links":0,"defined_names":32,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"AOS Switch Feature Matrix","index":0,"n_rows":352,"n_cols":21,"rows_kept":352,"cut":false,"hidden":false,"merged":[]}
[null," NetVanta AOS \nSwitch Feature Matrix\n\n      Updated: 11/18/2022\n• Supported (IPv4 Unless noted)\n—Not Supported or Not Applicable\nŦ Restrictions Apply\nŦ Dependent upon specific build\n","NV1224\n","NV1224 ST\n","NV1234\n1st Gen\n","NV1234\n2nd Gen\n","NV1234\n3rd Gen\n","NV1235P\n","NV1238\n1st Gen\n","NV1238\n2nd Gen\n","NV1238\n3rd Gen\n","NV1524ST\n","NV1531\n","NV1534\n2nd Gen\n","NV1535P\n","NV1544\n2nd Gen\n","NV1544F\n","NV1550-24\n","NV1550-48\n","NV1638\n","NV1748F\n"]
[null,"Part Number","1200500L1","1200504L1","170059xG1","170259xG1","170359xG1","170259xG1","170059xG1","170x59xG1","1703599G1","1200560L2","170057xF1","170259xGx","1702595G20","1702544Gx","1700546G1#120","17101524xF1","17101548xF1","4700568F1","1700558F1"]
[null,"Firmware: Initial Release","05.02.00","05.02.00","17.03.01","17.03.01","R11.2.0","R10.4.0","17.03.01","17.03.01","R11.2.0","09.01.00","R11.01.0","17.08.01","R10.4.0","17.08.01","17.05.01","BVS 1.0","BVS 1.0","18.01.01","DCSS 3.2"]
[null,"Firmware: Maintenance Release","13.13.00","13.13.00","18.01.00","R13.10.2","R13.10.2","R12.3.4","18.01.00","R13.10.2","R13.10.2","17.03.00","R14.1.2","R13.3.1","R12.3.4","R14.1.2","R14.1.2","R14.1.2","R14.1.2","R14.1.2","DCSS 3.2"]
[null,"Firmware: Feature Release",null,null,null,"R13.11.0","R13.11.0","R13.5.0",null,"R13.11.0","R13.11.0",null,"R14.1.0","R13.4.0","R13.5.0","R14.1.0","R14.1.0","R14.1.0","R14.1.0","R14.1.0"]
[null,"Status","Discontinued","Discontinued","Discontinued","Discontinued","Discontinued","Discontinued","Discontinued","Discontinued","Discontinued","Discontinued","Discontinued","Discontinued","Discontinued","Discontinued","Discontinued","Discontinued","Discontinued","Discontinued","Discontinued"]
[null,"Admin / Mgmt"]
[null,"Auto Configuration ","•","•","•","•","•","•","•","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"Cable Diagnostics ","—","—","•","•","•","•","•","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"CLI - Console Port","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"CLI - Telnet","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"CLI Privilege Level Access (7 Levels) ","7 levels","7 levels","7 levels","7 levels","7 levels","7 levels","7 levels","7 levels","7 levels","7 levels","7 levels","7 levels","7 levels","7 levels","7 levels","7 levels","7 levels","7 levels","7 levels"]
[null,"Cold start","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"CPU Load History  ","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"Daylight Saving","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"DDMI","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Desktop Auditing ","—","—","—","—","•","•","—","—","•","—","•","•","•","•","•","•","•","•","—"]
[null,"DHCP Network Forensics","—","—","—","—","•","•","—","—","•","—","•","•","•","•","•","—","—","•","—"]
[null,"EEE (Energy Efficient Ethernet)  Power Management","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Event History (Max Increased to 256KB) ","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"FM: Link Trace PDU (LTM) respond","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"FM: Loop Back PDU (LBM) respond","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"FTP Server","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—"]
[null,"Generic Email Client  ","—","—","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"HTTP Web Configuration ","•","•","•","•","•","IPv4/IPv6","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—"]
[null,"HTTPS","—","—","—","—","—","—","—","—","—","—",{"$f":"M268","v":"—"},"—","—",{"$f":"P268","v":"—"},{"$f":"Q268","v":"—"},{"$f":"R268","v":"—"},{"$f":"S268","v":"—"},"—","—"]
[null,"IPv4/IPv6 Ping","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"IPv4/IPv6 Traceroute","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"IPv6 Management","—","—","—","—","—","—","—","—","—","—",{"$f":"M151","v":"—"},"—","—",{"$f":"P151","v":"—"},{"$f":"Q151","v":"—"},{"$f":"R151","v":"—"},{"$f":"S151","v":"—"},"—","—"]
[null,"LED Power Management","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"LLDP (802.ab) ","—","—","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—"]
[null,"LLDP Inventory TLV  ","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"LLDP Ignore Speed Mismatch  ","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"LLDP-MED  ","—","—","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—"]
[null,"Loop detection restore to default","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Management access filtering","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"nCommand MSP Auto Link","•","•","•","•","•","•","•","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"Network Quality Monitoring ","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Network Time Protocol ","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"OAM HW Engine","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"On-the-fly SFP detection","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"PerfectReach","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC4884 (ICMPv6)","—","—","—","—","—","—","—","—","—","—",{"$f":"M154","v":"—"},"—","—",{"$f":"P154","v":"—"},{"$f":"Q154","v":"—"},{"$f":"R154","v":"—"},{"$f":"S154","v":"—"},"—","—"]
[null,"Ping -- Set TOS/DSCP and DF Flag ","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"Portal Lists ","—","—","•","•","•","IPv4/IPv6","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—"]
[null,"ProServices GUI ","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"RMON (Group 1, 2, 3 & 9)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RMON alarm and event(CLI,web)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 2613 SMON - PortCopy","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 3411 SNMP Management Frameworks","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 3414 User-based Security Model for SNMPv3","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 3415 View-based access Control Model for SNMP","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Safe Mode Download/RAM Disk","—","—","•","—","—","•","•","—","—","—","—","1702591G1","•","1702545G1","—","—","—","—","—"]
[null,"SFlow Export  ","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"SCP Client (Secure Copy) ","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"SCP Public Key Authentication (Secure Copy)","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"SFP Diagnostics ","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"SNMP V1 (No trap support)","•","•","•","•","•","IPv4/IPv6","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•"]
[null,"SNMP V2c","•","•","•","•","•","IPv4/IPv6","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•"]
[null,"SNMP V3 ","•","•","•","•","•","IPv4/IPv6","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•"]
[null,"SNMP Dying Gasp ","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"SNMP MIB OID","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"SNMP SFP Diagnostics ","—","—","—","—","•","•","—","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"SNMP FQDN as SNMP Trap Target ","—","—","—","—","•","•","—","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"SNMP Trap Buffering ","—","—","—","—","•","•","—","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"SSH CLI ","•","•","•","•","•","IPv4/IPv6","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•","•","IPv4/IPv6","•"]
[null,"SSHv2","—","—","—","—","—","—","—","—","—","—",{"$f":"M147","v":"—"},"—","—",{"$f":"P147","v":"—"},{"$f":"Q147","v":"—"},{"$f":"R147","v":"—"},{"$f":"S147","v":"—"},"—","—"]
[null,"SSH CLI 2048 bit Keys ","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"SSH CLI Public Key Authentication ","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"SSH Tunnel to Linux Server for Remote Access","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"SSL (HTTPS) Web Configuration ","•","•","•","•","•","IPv4/IPv6","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—"]
[null,"SSLv3 / TLS 1.0 (HTTPS) Web Configuration ","—","—","•","•","•","IPv4/IPv6","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","—"]
[null,"Switchport Scheduler","—","—","•","•","•","•","•","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"Symbolic Register Access","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Syslog","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Syslog for Congestion Fault Management","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"TCL Scripts","—","—","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—"]
[null,"Telnet CLI","•","•","•","•","•","IPv4/IPv6","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•"]
[null,"TFTP Server ","•","•","•","•","•","IPv4/IPv6","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•"]
[null,"Thermal Protection","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"TIA 1057 LLDP-MED","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Vitesse OAM Y.1731 PHY solution","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"VoIP Auto Configuration ","—","—","—","•","•","•","—","•","•","—","•","•","•","—","—","•","•","—","—"]
[null,"VoIP On Demand Report","—","—","—","•","•","•","—","•","•","—","•","•","•","—","—","•","•","—","—"]
[null,"Web & CLI Authentication","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"WLAN Automatic Security Key Generation ","—","—","•","•","•","•","•","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"WLAN Controller NetVanta 150","—","—","24 APs","24 APs","24 APs","24 APs","24 APs","24 APs","24 APs","—","8 APs","24 APs","24 APs","24 APs","24 APs","—","—","24 APs","—"]
[null,"WLAN Controller NetVanta 160","—","—","—","24 APs","24 APs","24 APs","—","24 APs","24 APs","—","8 APs","24 APs","24 APs","24 APs","24 APs","24 APs","24 APs","24 APs","—"]
[null,"IPv6 Features"]
[null,"Address Resolution ","—","—","—","—","•","•","—","—","•","—","•","•","•","•","•","•","•","•","—"]
[null,"Default Address Selection (Source Only)","—","—","—","—","•","•","—","—","•","—","•","•","•","•","•","•","•","•","—"]
[null,"Duplicate Address Detection ","—","—","—","—","•","•","—","—","•","—","•","•","•","•","•","•","•","•","—"]
[null,"Globally Change EtherType ","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"HW based IPv6 Static Routing","—","—","—","—","—","—","—","—","—","—",{"$f":"M225","v":"—"},"—","—",{"$f":"P225","v":"—"},{"$f":"Q225","v":"—"},{"$f":"R225","v":"—"},{"$f":"S225","v":"—"},"—","—"]
[null,"Jumbo Frame Support (bytes)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Named Prefixes ","—","—","—","—","•","•","—","—","•","—","•","•","•","•","•","•","•","•","—"]
[null,"Neighbor Discovery ","—","—","—","—","•","•","—","—","•","—","•","•","•","•","•","•","•","•","—"]
[null,"Neighbor Unreachability Detection","—","—","—","—","•","•","—","—","•","—","•","•","•","•","•","•","•","•","—"]
[null,"Multicast Listener Discovery (MLD) ","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Router Advertisement ","—","—","—","—","•","•","—","—","•","—","•","•","•","•","•","•","•","•","—"]
[null,"SW based IPv6 Static Routing","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Stateless Auto Configure (SLAAC)","—","—","—","—","•","•","—","—","•","—","•","•","•","•","•","•","•","•","—"]
[null,"Routing"]
[null,"ARP Cache Entries","—","—","—","232 Total","232 Total","232 Total","—","232 Total","232 Total","—","232 Total","232 Total","232 Total","512 Per Int.\n1000 Total","512 Per Int.\n1000 Total","1000 Total","1000 Total","512 Per Int.\n4100 Total","3072 Per Int.\n6144 Total"]
[null,"DHCP","•","•","•","•","•","IPv4/IPv6","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•"]
[null,"DHCP Client Option 60 ","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"DHCP Relay","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","•","•"]
[null,"DNS","•","•","•","•","•","IPv4/IPv6","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•"]
[null,"DNS Proxy","•","•","•","•","•","IPv4/IPv6","•","•","•","•","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","•"]
[null,"Dynamic DNS ","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—"]
[null,"HW based IPv4 Static Routing","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","—","—"]
[null,"IP source guard","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"IP subnet-based VLAN","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"OSPF v3","—","—","—","—","—","—","—","—","—","—","—","—","—","IPv4 Only","IPv4 Only","—","—","IPv4 Only","•"]
[null,"OSPF Distribute Lists ","—","—","—","•","•","•","—","•","•","—","•","•","•","IPv4 Only","IPv4 Only","•","•","IPv4 Only","•"]
[null,"PTP over IPv4","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 1035 DNS client, relay","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 2131 DHCP Client","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 2131 DHCP Server","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 2328 OSPFv2 Dynamic routing","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 3315 DHCPv6 Client","—","—","—","—","—","—","—","—","—","—",{"$f":"M232","v":"—"},"—","—",{"$f":"P232","v":"—"},{"$f":"Q232","v":"—"},{"$f":"R232","v":"—"},{"$f":"S232","v":"—"},"—","—"]
[null,"SW based IPv4 Static routing","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"UPNP","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"VRRP ","—","—","—","—","—","—","—","—","—","—","—","—","—","IPv4 Only","IPv4 Only","—","—","IPv4 Only","•"]
[null,"VRRP for VoIP ","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","—","—","•","•"]
[null,"Switching"]
[null,"ACLs for filtering/policing/port copy","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"ActivChassis (Stacking)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—"]
[null,"ActivReach ","—","—","—","—","—","•","—","—","—","—","—","—","•","—","—","—","—","—","—"]
[null,"AGGR/LACP user interface alignment with Industry standard","—","—","—","—","—","—","—","—","—","—",{"$f":"M224","v":"—"},"—","—",{"$f":"P224","v":"—"},{"$f":"Q224","v":"—"},{"$f":"R224","v":"—"},{"$f":"S224","v":"—"},"—","—"]
[null,"ARP inspection","—","—","—","—","—","—","—","—","—","—",{"$f":"M157","v":"—"},"—","—",{"$f":"P157","v":"—"},{"$f":"Q157","v":"—"},{"$f":"R157","v":"—"},{"$f":"S157","v":"—"},"—","—"]
[null,"Auto MAC addr. Learning/Ageing","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Bidirectional VLAN translation","—","—","—","—","—","—","—","—","—","—",{"$f":"M157","v":"—"},"—","—",{"$f":"P157","v":"—"},{"$f":"Q157","v":"—"},{"$f":"R157","v":"—"},{"$f":"S157","v":"—"},"—","—"]
[null,"Boundary Clock","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"BPDU Guard & Restricted Role","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Clock Quality","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Clustering (Single IP Address Management) ","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Combined SyncE & 1588","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"DHCP snooping","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"DiffServ (RFC2474) remarking","—","—","—","—","—","—","—","—","—","—",{"$f":"M236","v":"—"},"—","—",{"$f":"P236","v":"—"},{"$f":"Q236","v":"—"},{"$f":"R236","v":"—"},{"$f":"S236","v":"—"},"—","—"]
[null,"DiffServ to COS Mapping ","•","•","•","•","•","•","•","•","•","—","•","•","•","•","•","•","•","•","•"]
[null,"End-to-end transparent clock","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"EPS/ERPS using ETH-CCM","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Error Disable Recovery","—","—","—","—","—","—","—","—","—","—",{"$f":"M157","v":"—"},"—","—",{"$f":"P157","v":"—"},{"$f":"Q157","v":"—"},{"$f":"R157","v":"—"},{"$f":"S157","v":"—"},"—","—"]
[null,"Flow Control 802.3x ","—","—","—","—","—","—","—","—","—","—","•","•","—","•","•","•","•","•","•"]
[null,"Flow mirroring","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Flow OAM: Ingress/Egress","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"FM: Alarm indication signal (ETH-AIS)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"FM: Automatic Protection Switching (ETH-APS + ETH-RAPS)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"FM: CFM Dynamic TLV","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"FM: Continuity Check & Remote Defect Indication (ETH-CC + ETH-RDI)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"FM: Link trace (ETH-LT)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"FM: Locked Signal (ETH-LCK)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"FM: Loopback (ETH-LB )","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"FM: Test signal (ETH-Test)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Global Storm Control for UC, MC and BC","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Global/VCAP (ACL) policers","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Guest Default VLAN for Non-802.1x Devices ","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"Guest VLAN","—","—","—","—","—","—","—","—","—","—",{"$f":"M205","v":"—"},"—","—",{"$f":"P205","v":"—"},{"$f":"Q205","v":"—"},{"$f":"R205","v":"—"},{"$f":"S205","v":"—"},"—","—"]
[null,"GVRP ","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","—"]
[null,"G.781 compliant clock selection algorithm for the platform as a PTP slave","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"G.8031: 1:1 Port protection","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"G.8032 Ring protection","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"G.8032 Ring protection v. 2","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"G.8265.1 BMCA","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"G.8265 Compliant filter: Requires ZLS30380 network synchronization algorithm","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"G.8275.1 BMCA","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"G.8275 Compliant Filter: ZLS30380","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Hardware ACLs","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"IEEE-802.1ad Provider Bridge (Native or Translated VLAN)","—","—","—","—","—","—","—","—","—","—",{"$f":"M140","v":"—"},"—","—",{"$f":"P140","v":"—"},{"$f":"Q140","v":"—"},{"$f":"R140","v":"—"},{"$f":"S140","v":"—"},"—","—"]
[null,"IGMP Groups (Channels)","—","—","—","100","100","100","—","100","100","—","100","100","100","100","100","100","100","100","4K"]
[null,"IGMP Snooping ","•","•","•","•","•","•","•","•","•","—","•","—","•","—","—","•","•","•","•"]
[null,"IGMP Snooping Immediate Leave ","—","—","—","•","•","•","—","•","•","—","•","—","•","—","—","•","•","•","•"]
[null,"IGMPv2 snooping","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"IGMPv3 snooping","—","—","—","—","—","—","—","—","—","—",{"$f":"M157","v":"—"},"—","—",{"$f":"P157","v":"—"},{"$f":"Q157","v":"—"},{"$f":"R157","v":"—"},{"$f":"S157","v":"—"},"—","—"]
[null,"IGMP Querier ","—","—","—","•","•","•","—","•","•","—","•","—","•","—","—","•","•","•","•"]
[null,"IGMP Subscribers ","—","—","—","200","200","200","—","200","200","—","200","200","200","200","200","200","200","100 (w/ActivCh)","8K"]
[null,"IGMP filtering profile","—","—","—","—","—","—","—","—","—","—",{"$f":"M140","v":"—"},"—","—",{"$f":"P140","v":"—"},{"$f":"Q140","v":"—"},{"$f":"R140","v":"—"},{"$f":"S140","v":"—"},"—","—"]
[null,"Input priority mapping","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"IPMC throttling, filtering, leave proxy","—","—","—","—","—","—","—","—","—","—",{"$f":"M249","v":"—"},"—","—",{"$f":"P249","v":"—"},{"$f":"Q249","v":"—"},{"$f":"R249","v":"—"},{"$f":"S249","v":"—"},"—","—"]
[null,"iPVLAN Trunking","—","—","—","—","—","—","—","—","—","—",{"$f":"M157","v":"—"},"—","—",{"$f":"P157","v":"—"},{"$f":"Q157","v":"—"},{"$f":"R157","v":"—"},{"$f":"S157","v":"—"},"—","—"]
[null,"ITU filtering: ZLS30380 servo network synchronization algorithm","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Jumbo Frames (MTU) ","—","—","2K","2K","2K","9K","2K","2K","2K","—","9K","9K","9K","13K","13K","9K","9K","12K","9K"]
[null,"LACP loop free operation","—","—","—","—","—","—","—","—","—","—",{"$f":"M249","v":"—"},"—","—",{"$f":"P249","v":"—"},{"$f":"Q249","v":"—"},{"$f":"R249","v":"—"},{"$f":"S249","v":"—"},"—","—"]
[null,"LACP Revertive/Non-revertive","—","—","—","—","—","—","—","—","—","—",{"$f":"M140","v":"—"},"—","—",{"$f":"P140","v":"—"},{"$f":"Q140","v":"—"},{"$f":"R140","v":"—"},{"$f":"S140","v":"—"},"—","—"]
[null,"Layer 3 Switching","—","—","—","L3 Lite","L3 Lite","L3 Lite","—","L3 Lite","L3 Lite","—","L3 Lite","L3 Lite","L3 Lite","•","•","L3 Lite","L3 Lite","•","•"]
[null,"Layer 3 Switching Interfaces","—","—","—","16","16",8,"—","16","16","—",8,8,8,128,128,"16","16",256,"4K"]
[null,"Layer 3 Switching Routes","—","—","—","32","32",16,"—","32","32","—",16,16,16,1000,1000,"32","32",2000,"4K"]
[null,"Link Aggregation (802.3ad) ","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Link Aggregation LACP","—","—","—","—","—","—","—","—","—","—",{"$f":"M157","v":"—"},"—","—",{"$f":"P157","v":"—"},{"$f":"Q157","v":"—"},{"$f":"R157","v":"—"},{"$f":"S157","v":"—"},"—","—"]
[null,"Link Aggregation Static","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Link State Tracking","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Loop Guard","—","—","—","—","—","—","—","—","—","—",{"$f":"M242","v":"—"},"—","—",{"$f":"P242","v":"—"},{"$f":"Q242","v":"—"},{"$f":"R242","v":"—"},{"$f":"S242","v":"—"},"—","—"]
[null,"MAC Addresses - Static","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"MAC Authentication Bypass ","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"MAC-Based Authentication","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"MAC-based VLAN","—","—","—","—","—","—","—","—","—","—",{"$f":"M249","v":"—"},"—","—",{"$f":"P249","v":"—"},{"$f":"Q249","v":"—"},{"$f":"R249","v":"—"},{"$f":"S249","v":"—"},"—","—"]
[null,"MAC Table Entries","8K","8K","8K","8K","8K","8K","8K","8K","8K","8K","8K","8K","8K","16K","16K","16K","16K","32K","64K"]
[null,"MLDv1 snooping","—","—","—","—","—","—","—","—","—","—",{"$f":"M224","v":"—"},"—","—",{"$f":"P224","v":"—"},{"$f":"Q224","v":"—"},{"$f":"R224","v":"—"},{"$f":"S224","v":"—"},"—","—"]
[null,"MLDv2 snooping","—","—","—","—","—","—","—","—","—","—",{"$f":"M236","v":"—"},"—","—",{"$f":"P236","v":"—"},{"$f":"Q236","v":"—"},{"$f":"R236","v":"—"},{"$f":"S236","v":"—"},"—","—"]
[null,"MSCC Timing BU servo algorithm integration (MSCC ZLS30387)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"MSCC Timing BU DPLL API integration","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"MSTP","—","—","—","—","—","—","—","—","—","—",{"$f":"M249","v":"—"},"—","—",{"$f":"P249","v":"—"},{"$f":"Q249","v":"—"},{"$f":"R249","v":"—"},{"$f":"S249","v":"—"},"—","—"]
[null,"Multiple Registration Protocol MRP","—","—","—","—","—","—","—","—","—","—",{"$f":"M224","v":"—"},"—","—",{"$f":"P224","v":"—"},{"$f":"Q224","v":"—"},{"$f":"R224","v":"—"},{"$f":"S224","v":"—"},"—","—"]
[null,"Multiple VLAN Registration Protocol MVRP","—","—","—","—","—","—","—","—","—","—",{"$f":"M236","v":"—"},"—","—",{"$f":"P236","v":"—"},{"$f":"Q236","v":"—"},{"$f":"R236","v":"—"},{"$f":"S236","v":"—"},"—","—"]
[null,"MVR","—","—","—","—","—","—","—","—","—","—",{"$f":"M242","v":"—"},"—","—",{"$f":"P242","v":"—"},{"$f":"Q242","v":"—"},{"$f":"R242","v":"—"},{"$f":"S242","v":"—"},"—","—"]
[null,"MVR profile","—","—","—","—","—","—","—","—","—","—",{"$f":"M132","v":"•"},"—","—",{"$f":"P132","v":"•"},{"$f":"Q132","v":"•"},{"$f":"R132","v":"•"},{"$f":"S132","v":"•"},"—","—"]
[null,"Nested MEPs","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"OAM inject engine support","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"OAM inject engine support 2","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Peer-to-peer transparent clock","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"PM: Dual Ended Frame Loss Measurement - CCM based (ETH-LM)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"PM: Frame delay and delay variation measurement (ETH-DM)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"PM: Single Ended Frame Loss Measurement LMM/LMR based (ETH-LM)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"PoE-802.3af ","1200580L1","1200584L1","1700595G1","1702595G1","1702595G1","•","1700599G1","1702599G1","1702599G1","—","1700571F1","1702591G1","•","1702545G1","—","17101524PF1","17101548PF1","4700569F1","—"]
[null,"PoE-802.3at ","—","—","—","—","—","—","—","—","—","—","1700571F1","1702591G1","—","1702545G1","—","17101524PF1","17101548PF1","4700569F1","—"]
[null,"PoE-Legacy ","—","—","1700595G1","1702595G1","1702595G1","•","1700599G1","1702599G1","1702599G1","—","1700571F1","1702591G1","•","1702545G1","—","17101524PF1","17101548PF1","4700569F1","—"]
[null,"POE/POE+ - PD69208 Support","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"POE/POE+ with LLDP","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Port Authentication 802.1x Supplicant Mode ","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Port Authentication 802.1x Authenticator Mode","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Port Authentication 802.1x on Trunk Ports & Voice VLAN Ports ","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","•","•"]
[null,"Port Default Priority","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Port egress shaper","—","—","—","—","—","—","—","—","—","—",{"$f":"M157","v":"—"},"—","—",{"$f":"P157","v":"—"},{"$f":"Q157","v":"—"},{"$f":"R157","v":"—"},{"$f":"S157","v":"—"},"—","—"]
[null,"Port Isolation Static","—","—","—","—","—","—","—","—","—","—",{"$f":"M140","v":"—"},"—","—",{"$f":"P140","v":"—"},{"$f":"Q140","v":"—"},{"$f":"R140","v":"—"},{"$f":"S140","v":"—"},"—","—"]
[null,"Port Mirroring","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Port policers","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Port Security (MAC Based) ","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Private VLAN Static","—","—","—","—","—","—","—","—","—","—",{"$f":"M236","v":"—"},"—","—",{"$f":"P236","v":"—"},{"$f":"Q236","v":"—"},{"$f":"R236","v":"—"},{"$f":"S236","v":"—"},"—","—"]
[null,"Protocol-based VLAN","—","—","—","—","—","—","—","—","—","—",{"$f":"M242","v":"—"},"—","—",{"$f":"P242","v":"—"},{"$f":"Q242","v":"—"},{"$f":"R242","v":"—"},{"$f":"S242","v":"—"},"—","—"]
[null,"Protected Ports (Private VLAN Edge) ","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"PTP Profile","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"PTP Time Interface","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"QoS Assignment","—","—","—","—","—","—","—","—","—","—",{"$f":"M204","v":"—"},"—","—",{"$f":"P204","v":"—"},{"$f":"Q204","v":"—"},{"$f":"R204","v":"—"},{"$f":"S204","v":"—"},"—","—"]
[null,"QoS Control List (QCL Mode)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Queue egress shapers","—","—","—","—","—","—","—","—","—","—",{"$f":"M224","v":"—"},"—","—",{"$f":"P224","v":"—"},{"$f":"Q224","v":"—"},{"$f":"R224","v":"—"},{"$f":"S224","v":"—"},"—","—"]
[null,"Queue policers","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Random Early Discard (RED)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Rapid Spanning Tree ","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Redundant masters and multiple timing domains","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Rmirror","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Scheduler mode","—","—","—","—","—","—","—","—","—","—",{"$f":"M249","v":"—"},"—","—",{"$f":"P249","v":"—"},{"$f":"Q249","v":"—"},{"$f":"R249","v":"—"},{"$f":"S249","v":"—"},"—","—"]
[null,"Spanning Tree","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Spanning Tree Root Guard ","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","•","•"]
[null,"Storm Control","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","•","•"]
[null,"Storm Control (Enhanced) ","—","—","—","—","—","—","—","—","—","—","•","—","—","—","—","•","•","—","—"]
[null,"SyncE Nomination For 2 Interfaces","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"SyncE with SSM","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Tag remarking","—","—","—","—","—","—","—","—","—","—",{"$f":"M140","v":"—"},"—","—",{"$f":"P140","v":"—"},{"$f":"Q140","v":"—"},{"$f":"R140","v":"—"},{"$f":"S140","v":"—"},"—","—"]
[null,"TC internal Master/Slave w. PDV filtering","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"TC internal Master/Slave w. reduced PDV filtering","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Traffic Classes (8 active priorities)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"UDLD","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Unidirectional VLAN translation (ingress/egress)","—","—","—","—","—","—","—","—","—","—",{"$f":"M224","v":"—"},"—","—",{"$f":"P224","v":"—"},{"$f":"Q224","v":"—"},{"$f":"R224","v":"—"},{"$f":"S224","v":"—"},"—","—"]
[null,"UNI LAG (LACP) 1:1 Active/Standby","—","—","—","—","—","—","—","—","—","—",{"$f":"M236","v":"—"},"—","—",{"$f":"P236","v":"—"},{"$f":"Q236","v":"—"},{"$f":"R236","v":"—"},{"$f":"S236","v":"—"},"—","—"]
[null,"User Priority","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Virtual LAN","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"VLAN Assignment","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"VLAN Aware Port Security ","—","—","•","•","•","•","•","•","•","—","•","•","•","•","•","•","•","•","•"]
[null,"VLAN Interface ","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"VLAN Support (802.1Q)","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"VLAN Trunking","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Voice VLAN","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"802.1Qbb Per Priority Flow Control","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"802.3ah: Variable, request, response","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"802.3ah: Discovery process, information. Event notification, loopback","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"802.3ah: Dying Gasp","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"802.3ah: Dying Gasp SNMP Trap","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"1588v2 PTP with two step clock","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"1588v2 PTP with one step clock","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Windows Machine Authentication/Port Authentication","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","•","•"]
[null,"Security"]
[null,"AAA Authentication","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"AAA with TACACS+ ","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Denial of Service (DoS) Protection ","—","—","—","—","—","•","—","—","—","—","•","•","•","•","•","•","•","•","•"]
[null,"IP MAC binding","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"IP/MAC binding dynamic to static","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"MAC Address Limit","—","—","—","—","—","—","—","—","—","—","8K","—","—",null,null,"16K","16K","—","—"]
[null,"Multiple 802.1X","—","—","—","—","—","—","—","—","—","—",{"$f":"M131","v":"—"},"—","—",{"$f":"P131","v":"—"},{"$f":"Q131","v":"—"},{"$f":"R131","v":"—"},{"$f":"S131","v":"—"},"—","—"]
[null,"Port-Based 802.1X","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RADIUS Accounting","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RADIUS Authentication and Authorization","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Security Audit ","—","—","•","•","•","•","•","•","•","—","•","•","•","•","•","•","•","•","—"]
[null,"Single 802.1X","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"TACACS+ Accounting","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"TACACS+ Authentication and Authorization","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"TACACS+ Command Authorization","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"SFPs / SFP Cables"]
[null,"1000BaseLX -- 1310nm SFP (1200481E1)","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"1000BaseSX -- 850nm SFP (1200480E1)","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Enhanced 2.5 Gbps Multimode SFP (1200482G1)","—","—","—","•","•","•","—","•","•","—","—","•","•","•","•","—","—","•","•"]
[null,"Enhanced 2.5 Gbps Singlemode SFP (1200483G1)","—","—","—","•","•","•","—","•","•","—","—","•","•","•","•","—","—","•","•"]
[null,"1000BaseT Ethernet SFP (1200485G1)","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","•","•","—","•"]
[null,"10GBase-SR SFP+ Transceiver (1700485F1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•"]
[null,"10GBase-LR SFP+ Transceiver (1700486F1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","•","•","•"]
[null,"1M Interconnect Cable SFP (1200484G1)","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","—","—","•","•"]
[null,"3M Interconnect Cable SFP (1200484G3)","—","—","—","•","•","•","—","•","•","—","•","•","•","•","•","—","—","•","•"]
[null,"1M Interconnect Cable SFP+ (1710484F1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","1/10 - Gbps","1/10 - Gbps","•","•"]
[null,"3M Interconnect Cable SFP+ (1710484F3)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","1/10 - Gbps","1/10 - Gbps","•","•"]
[null,"5M Interconnect Cable SFP+ (1710484F5)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","1/10 - Gbps","1/10 - Gbps","•","•"]
[null,"Modules"]
[null,"Dual SFP XIM Module (1700473F1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—"]
[null,"Dual SFP+ XIM Module (1700471F1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—"]
[null,"Stacking XIM (1700470F1)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","•","—"]
[null,"Physical Specifications"]
[null,"Chassis Weight","7lbs","7lbs","Ŧ 5lbs - 10lbs","Ŧ 5lbs - 10lbs","Ŧ 5lbs - 12.7lbs","9.5lbs","Ŧ 8.5lbs - 12.5lbs","Ŧ 8.5lbs - 13.5lbs","Ŧ 8.5lbs - 13.5lbs","7lbs","3.5lbs","4lbs - 9.5lbs","9.5lbs","4lbs - 9.5lbs","6lbs - 9.5lbs","5lbs - 9.5lbs","8lbs - 10.5lbs","11.5lbs","TBD"]
[null,"Ethernet Switch Ports (Copper)","24 - 10/100","24 - 10/100\n2 - 10/100/1000","24 - 10/100\n2 - 10/100/1000","24 - 10/100\n2 - 10/100/1000","24 - 10/100\n2 - 10/100/1000","24 - 10/100","48 - 10/100\n2 - 10/100/1000","48 - 10/100\n2 - 10/100/1000","48 - 10/100\n2 - 10/100/1000","28 - 10/100/1000","10 - 10/100/1000","24 - 10/100/1000","24 - 10/100/1000","24 - 10/100/1000","—","24 - 10/100/1000","48 - 10/100/1000","48 - 10/100/1000","—"]
[null,"Ethernet Switch Ports (Fiber SFP Slots)","—","2 Combo","2 Combo","2 Combo\n2 Enhanced","2 Combo\n2 Enhanced","2 Standard\n2 Enhanced","2 Combo","2 Combo\n2 Enhanced","2 Combo\n2 Enhanced","4 Standard 1 Gbps  SFPs","2 Standard 1 Gbps SFPs","2 Standard 1 Gbps  SFPs  & 2 Enhanced 1/2.5 Gbps SFPs","2 Standard 1 Gbps  SFPs  & 2 Enhanced 1/2.5 Gbps SFPs","4 Enhanced 1/2.5 Gbps SFPs","24 Standard 1 Gbps  SFPs  & 2 Enhanced 1/2.5 Gbps SFPs","4 Enhanced 1/10 Gbps SFP+","4 Enhanced 1/10 Gbps SFP+","Requires XIM","48-1/10Gbps SFP+\n4-40Gbps (Future)"]
[null,"Flash Size","8MB","8MB","8MB","8MB","8MB","32MB","8MB","8MB","8MB","—","32MB","32MB","32MB","32MB","32MB","128MB","128MB","128MB","TBD"]
[null,"Internal Fan(s)","TBD","TBD","TBD","TBD","• 2x (PoE Only)","• 2x","TBD","—","• 2x","TBD","—","• 1x\n• 2x (PoE)","• 2x","• 1x\n• 2x (PoE)","• 2x","• 1x\n• 3x (PoE)","• 1x\n• 3x (PoE)","• 4x\n• 4x (PoE)","• 4x"]
[null,"Mean Time Between Failure (MTBF)","273,001 Hrs","249,564 Hrs","329,148 Hrs","329,148 Hrs","541,571 Hrs","184,253 Hrs","329,148 Hrs","329,148 Hrs","351,133 Hrs","189,538 Hrs","324,197 Hrs","418,756 Hrs","418,756 Hrs","820,143 Hrs","527,449 Hrs","TBD","TBD","367,926 Hrs","TBD"]
[null,"Micro USB Port ","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Operating Temperature (relative humidity up to 95% non-Condensing)","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 122°F","32°F to 104°F"]
[null,"Rack Mount Dimensions","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U 1/2 Rack, 19\"","1U, 1/2 Rack, 19\"","1U, 19\"","1U 1/2 Rack, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\""]
[null,"RAM Size","16MB","16MB","64MB","64MB","64MB","128MB","64MB","64MB","64MB","—","128MB","128MB","128MB","128MB","128MB","256MB","256MB","256MB","TBD"]
[null,"RAM Upgrade Capacity","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","1GB","—"]
[null,"USB Port(s)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","Ŧ ","Ŧ "]
[null,"Power"]
[null,"AC Power Supply","100–250 VAC","100–250 VAC","100–250 VAC","100–250 VAC","100–250 VAC","100–250 VAC","100–250 VAC","100–250 VAC","100–250 VAC","100–250 VAC","100–250 VAC","100–250 VAC","100–250 VAC","100–250 VAC","120 VAC","100–240 VAC","100–240 VAC","110–230 VAC","100–240 VAC\n(2x PSU's Hot Swappable)"]
[null,"DC Power Supply","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","Future"]
[null,"EPS Support","—","—","—","—","—","•","—","—","—","—","—","•","•","•","—","—","—","•","—"]
[null,"Max BTU",86,86,86,86,86,"1700",138,138,138,122,103,103,103,103,275,"68","205","550","TBD"]
[null,"Max BTU with PoE Ŧ",1550,1550,775,775,775,"1700",1720,1720,1720,"—","—","—","—",1720,"—","1570","1570","1800","—"]
[null,"Max Wattage","25W","25W","25W","25W","25W","25W","40W","40W","40W","36W","30W","30W","—","30W","80W","20W","60W","160W","165W"]
[null,"Max Wattage with PoE Ŧ","500W","500W",null,"500W","500W","500W","500W","500W","500W","—","95W","500W","500W","500W","—","460W","460W","630W","—"]
[null,"PoE Power Budget","370W","370W","185W","370W","370W","370W","370W","370W","370W","—","65W","370W","370W","370W","—","370W","370W","370W","—"]
[null,"RPS Support","—","—","—","—","—","•","—","—","—","—","—","1702591G1","•","1702545G1","—","—","—","4700569F1","—"]
[null,"MIBs "]
[null,"IEEE 802.1 MSTP MIB","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"IEEE 802.1AB LLDP-MIB (LLDP MIB included in a clause of the STD)","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"IEEE 802.1Q Bridge MIB 2008","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•","•"]
[null,"IEEE 802.1X (PAE MIB included in a clause of the STD)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"IEEE 802.3ad (LACP MIB included in a clause of the STD)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Private MIB framework","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 1213 MIB II","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 1215 TRAPS MIB","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 1850 OSPF Version 2 MIB","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 2674 VLAN MIB","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 2819 RMON (Group 1, 2. 3 & 9)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 2863 Interface Group MIB using SMI v2","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 3621 LLDP-MED Power (POE) (No specific MIB for POE+ exists)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 3635 Ethernet-like MIB","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 3636 802.3 MAU MIB","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 4133 Entity MIB version 3","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 4188 Bridge MIB","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 4292 IP Forwarding Table MIB","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 4293 Management Information Base for the Internet Protocol (IP)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 4668 RADIUS auth. Client MIB","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 4670 RADIUS Accounting MIB","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 4878 Link OAM MIB","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RFC 5519 Multicast Group Membership Discovery MIB","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]
[null,"TIA 1057 LLDP-MED ( MIB is part of the STD)","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—","—"]