{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Switch Feature Matrix"],"not_rendered":{"charts":0,"images":29,"macros":1,"external_links":0,"defined_names":41,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Switch Feature Matrix","index":0,"n_rows":300,"n_cols":13,"rows_kept":300,"cut":false,"hidden":false,"merged":[]}
[null,"\n      ","1560-08","1560-08-65W","1560-08-150W","1560-24","1560-24-370W","1560-24-740W","1560-48","1560-48-370W","1560-48-740W","1570-24-370W","1760-12F"]
[null,"Part Number","17101561F1","17101561PF2","17108108PF2","17101564F1","17101564PF2","17108124PF2","17101568F1","17101568PF2","17108148PF2","17101574PF1","17101763F1"]
[null,"Firmware: Initial Release"," 4.4-45"," 4.4-41"," 4.4-41"," 4.4-45"," 4.4-41"," 4.4-41"," 4.4-45"," 4.4-41"," 4.4-41","v20.12-3","v20.12-3"]
[null,"Firmware: Maintenance Release"," 4.4-47"," 4.4-47"," 4.4-47"," 4.4-47"," 4.4-47"," 4.4-47"," 4.4-47"," 4.4-47"," 4.4-47","v20.12-3","v20.12-3"]
[null,"Firmware: Feature Release"," 4.4-47"," 4.4-47"," 4.4-47"," 4.4-47"," 4.4-47"," 4.4-47"," 4.4-47"," 4.4-47"," 4.4-47","v20.12-3","v20.12-3"]
[null,"Operating System ","ASE","ASE","ASE","ASE","ASE","ASE","ASE","ASE","ASE","ASE","ASE"]
[null,"Management"]
[null,"Remote VLAN Monitor (RMirror)","•","•","•","•","•","•","•","•","•","•","—"]
[null,"Alarm Module","•","•","•","•","•","•","•","•","•","•","•"]
[null,"CLI - Telnet ","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6"]
[null,"CLI - SSH (SSHV2)","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6"]
[null,"CLI - Console Port","•","•","•","•","•","•","•","•","•","•","•"]
[null,"CLI Privilege Level Access"," 15 levels"," 15 levels"," 15 levels"," 15 levels"," 15 levels"," 15 levels"," 15 levels"," 15 levels"," 15 levels"," 15 levels"," 15 levels"]
[null,"Daylight Saving","•","•","•","•","•","•","•","•","•","•","•"]
[null,"HTTP Web Configuration ","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6"]
[null,"HTTPS Web Configuration ","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6"]
[null,"IPv4/IPv6 Traceroute","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Management Access Filtering","•","•","•","•","•","•","•","•","•","•","•"]
[null,"nCommand MSP Auto Link","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC4884 ICMPv6","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Remote Network Monitoring RMON (Group 1, 2, 3 & 9)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Remote Network Monitoring  RMON alarm and event (CLI,web)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"sFlow Export  ","•","•","•","•","•","•","•","•","•","•","•"]
[null,"SNMP V1 (No trap support)","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6"]
[null,"SNMP V2c","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6"]
[null,"SNMP V3 ","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6"]
[null,"Syslog","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Universal Plug and Play (UPnP)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Port Mirroring","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Secure FTP (SFTP) Client","—","—","—","—","—","—","—","—","—","•","•"]
[null,"Telnet Client","—","—","—","—","—","—","—","—","—","•","•"]
[null,"SSH Client","—","—","—","—","—","—","—","—","—","•","•"]
[null,"HTTPS Custom Certificates","•","•","•","•","•","•","•","•","•","•","•"]
[null,"IPv4/IPv6 Ping","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Layer 2"]
[null,"Virtual LAN","•","•","•","•","•","•","•","•","•","•","•"]
[null,"802.ab LLDP  ","•","•","•","•","•","•","•","•","•","•","•"]
[null,"TIA 1057 LLDP-MED  ","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Jumbo Frame Support (bytes)",10240,10240,10240,10240,10240,10240,10240,10240,10240,10240,10240]
[null,"IP Source Guard","•","•","•","•","•","•","•","•","•","IPv4/IPv6","IPv4/IPv6"]
[null,"VLAN Translation Bidirectional","•","•","•","•","•","•","•","•","•","•","•"]
[null,"BPDU Guard & Restricted Role","•","•","•","•","•","•","•","•","•","•","•"]
[null,"GARP VLAN Registration Protocol (GVRP)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Shard VLAN Learning (SVL)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"802.3ad Link Aggregation (LACP)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"LACP Loop Free Operation","•","•","•","•","•","•","•","•","•","•","•"]
[null,"LACP Revertive/Non-revertive","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Link Aggregation Static","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Loop Protection","•","•","•","•","•","•","•","•","•","•","•"]
[null,"MAC-based VLAN","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Multiple Spanning Tree (MSTP)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Multiple Registration Protocol (MRP/MVRP)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Private VLAN","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Port Isolation ","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Protocol-Based VLAN","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Rapid Spanning Tree (RSTP) ","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Spanning Tree (STP)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Spanning Tree Root Guard ","•","•","•","•","•","•","•","•","•","•","•"]
[null,"VLAN Translation Unidirectional (ingress/egress)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"802.1q VLAN Trunking ","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Voice VLAN","•","•","•","•","•","•","•","•","•","•","•"]
[null,"S-Tag Support QinQ","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Static MAC Address Support","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Port Control"]
[null,"Cable Diagnostics ","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Digital Diagnostics Monitoring Interface (DDMI)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"SFP Diagnostics ","•","•","•","•","•","•","•","•","•","•","•"]
[null,"802.3x Flow Control ","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Port Speed ","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Port Duplex","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Uni Directional Link Detection (UDLD)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"802.1Qbb Priority Flow Control","•","•","•","•","•","•","•","•","•","•","—"]
[null,"Layer 3"]
[null,"IPv6 Static Routing","•","•","•","•","•","•","•","•","•","•","•"]
[null,"OSPFv2","—","—","—","—","—","—","—","—","—","—","—"]
[null,"OSPFv3","—","—","—","—","—","—","—","—","—","—","—"]
[null,"RIP v1/v2","—","—","—","—","—","—","—","—","—","•","•"]
[null,"DHCP  Client","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6","IPv4/IPv6"]
[null,"DHCP Server","•","•","•","•","•","•","•","•","•","•","•"]
[null,"DHCP Relay","•","•","•","•","•","•","•","•","•","•","•"]
[null,"DHCP Option 82 Relay (Information Mode)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"DNS Proxy","•","•","•","•","•","•","•","•","•","•","•"]
[null,"IPv4 Static Routing","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Interaface VLANs","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Custom DHCP Server Options","•","•","•","•","•","•","•","•","•","•","•"]
[null,"QoS"]
[null,"Storm Control for Unicast, Broadcast, Multicast","•","•","•","•","•","•","•","•","•","•","•"]
[null,"DiffServ Marking/Remarking","•","•","•","•","•","•","•","•","•","•","•"]
[null,"DiffServ to COS Mapping ","•","•","•","•","•","•","•","•","•","•","•"]
[null,"COS Marking/Remarking","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Rate Limiting","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Ingress Priority Mapping","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Port Default Priority","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Per Port  Shaper","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Per Port Policers","•","•","•","•","•","•","•","•","•","•","•"]
[null,"QoS Control List (QCL)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Per Queue Shapers","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Per Queue Policers","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Random Early Discard (RED)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Traffic Classes (8 Queues)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Scheduler WRR/Strict Priority","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Queue cut-through","—","—","—","—","—","—","—","—","—","•","•"]
[null,"TSN - 802.1Qbv Time-Aware Scheduler (TAS)","—","—","—","—","—","—","—","—","—","—","•"]
[null,"TSN - 802.1Qbu & 802.3br Frame Preemption","—","—","—","—","—","—","—","—","—","—","•"]
[null,"TSN - 802.1Qci  Per-Stream Filtering and Policing (PSFP)","—","—","—","—","—","—","—","—","—","—","•"]
[null,"Multicast "]
[null,"Multicast VLAN Registration (MVR)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"IGMP Snooping Fast Leave ","•","•","•","•","•","•","•","•","•","•","•"]
[null,"IGMP Snooping ","•","•","•","•","•","•","•","•","•","•","•"]
[null,"IGMP v1","•","•","•","•","•","•","•","•","•","•","•"]
[null,"IGMP v2","•","•","•","•","•","•","•","•","•","•","•"]
[null,"IGMP v3","•","•","•","•","•","•","•","•","•","•","•"]
[null,"IGMP Filtering Profile","•","•","•","•","•","•","•","•","•","•","•"]
[null,"MLD Snooping  ","•","•","•","•","•","•","•","•","•","•","•"]
[null,"MLDv1","•","•","•","•","•","•","•","•","•","•","•"]
[null,"MLDv2","•","•","•","•","•","•","•","•","•","•","•"]
[null,"MLD Querier","•","•","•","•","•","•","•","•","•","•","•"]
[null,"MLD Fast Leave","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Multicast Throttling, Filtering, Proxy, Leave Proxy","•","•","•","•","•","•","•","•","•","•","•"]
[null,"IGMP Querier ","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Security"]
[null,"DHCP Snooping","•","•","•","•","•","•","•","•","•","•","•"]
[null,"ARP Inspection","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Guest VLAN","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Access Control Lists (ACL)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"MAC-Based Authentication","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RADIUS Assigned VLAN ","•","•","•","•","•","•","•","•","•","•","•"]
[null,"IP MAC Binding","•","•","•","•","•","•","•","•","•","•","•"]
[null,"IP/MAC Binding Dynamic to Static","•","•","•","•","•","•","•","•","•","•","•"]
[null,"MAC Address Limit","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Persistent MAC Learning (Sticky MAC)","—","—","—","—","—","—","—","—","—","•","•"]
[null,"Port-Based 802.1x","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Multiple 802.1x","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Single 802.1x","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RADIUS CoA VLAN Assignment","•","•","•","•","•","•","•","•","•"]
[null,"RADIUS Accounting","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RADIUS Authentication and Authorization","•","•","•","•","•","•","•","•","•","•","•"]
[null,"TACACS+ Accounting","•","•","•","•","•","•","•","•","•","•","•"]
[null,"TACACS+ Authentication and Authorization","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Port Security MAC addr. Limit/Ageing","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RADIUS Assigned QoS","•","•","•","•","•","•","•","•","•","•","•"]
[null,"AAA Authentication","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Ethernet Protection"]
[null,"G.8031 Ethernet Linear protection 1:1 (ELPS/APS)","•","•","•","•","•","•","•","•","•","—","•"]
[null,"G.8031 Ethernet Linear protection 1+1 Bidirectional (ELPS/APS)","•","•","•","•","•","•","•","•","•","—","•"]
[null,"G.8031 Ethernet Linear protection 1+1 Unidirectional (ELPS/APS)","—","—","—","—","—","—","—","—","—","—","•"]
[null,"TSN - 802.1cb Frame Replication and Elimination for Reliability (FRER)","—","—","—","—","—","—","—","—","—","—","•"]
[null,"G.8032 Ethernet Ring Protection (ERPS)","•","•","•","•","•","•","•","•","•","—","•"]
[null,"Ethernet OAM"]
[null,"Syslog for Congestion Fault Management","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Link State Tracking","•","•","•","•","•","•","•","•","•","—","—"]
[null,"CFM: ETH-CCM","•","•","•","•","•","•","•","•","•","—","•"]
[null,"Nested MEPs","•","•","•","•","•","•","•","•","•","—","—"]
[null,"PM: Dual Ended Frame Loss Measurement - CCM based (ETH-LM)","•","•","•","•","•","•","•","•","•","—","—"]
[null,"PM: Frame Delay and Delay Variation Measurement (ETH-DM)","•","•","•","•","•","•","•","•","•","—","—"]
[null,"PM: Single Ended Frame Loss Measurement LMM/LMR based (ETH-LM)","•","•","•","•","•","•","•","•","•","—","—"]
[null,"Flow OAM: Ingress/Egress","•","•","•","•","•","•","•","•","•","—","—"]
[null,"FM: Alarm Indication Signal (ETH-AIS)","•","•","•","•","•","•","•","•","•","—","—"]
[null,"FM: Automatic Protection Switching (ETH-APS + ETH-RAPS)","•","•","•","•","•","•","•","•","•","—","—"]
[null,"FM: CFM Dynamic TLV","•","•","•","•","•","•","•","•","•","—","—"]
[null,"FM: Continuity Check & Remote Defect Indication (ETH-CC + ETH-RDI)","•","•","•","•","•","•","•","•","•","—","—"]
[null,"FM: Link Trace (ETH-LT)","•","•","•","•","•","•","•","•","•","—","—"]
[null,"FM: Locked Signal (ETH-LCK)","•","•","•","•","•","•","•","•","•","—","—"]
[null,"FM: Loopback (ETH-LB )","•","•","•","•","•","•","•","•","•","—","—"]
[null,"FM: Test Signal (ETH-Test)","•","•","•","•","•","•","•","•","•","—","—"]
[null,"FM: Link Trace PDU (LTM) Respond","•","•","•","•","•","•","•","•","•","—","—"]
[null,"FM: Loop Back PDU (LBM) Respond","•","•","•","•","•","•","•","•","•","—","—"]
[null,"OAM HW Engine","—","—","—","•","•","•","•","•","•","—","•"]
[null,"802.3ah Variable, Request, Response","•","•","•","•","•","•","•","•","•","—","•"]
[null,"802.3ah Discovery Process, Information. Event Notification, Loopback","•","•","•","•","•","•","•","•","•","—","•"]
[null,"802.3ah Dying Gasp","•","•","•","•","•","•","•","•","•","—","•"]
[null,"802.3ah Dying Gasp Enhanced","—","—","—","—","—","—","—","—","—","—","•"]
[null,"802.3ah Dying Gasp SNMP Trap","•","•","•","•","•","•","•","•","•","—","•"]
[null,"CFM: IS-, OS-, PS-, SID-TLV","—","—","—","—","—","—","—","—","—","—","•"]
[null,"CFM: ASP using Eth-CCM and Eth-APS","—","—","—","—","—","—","—","—","—","—","•"]
[null,"CFM: ERPS using ETJ-CCM and ETH-RAPS","—","—","—","—","—","—","—","—","—","—","•"]
[null,"Timing & Synchronization"]
[null,"Redundant masters and multiple timing domains","•","•","•","•","•","•","•","•","•","—","•"]
[null,"SyncE Nomination For 2 Interfaces","•","•","•","•","•","•","•","•","•","—","—"]
[null,"SyncE with SSM","•","•","•","•","•","•","•","•","•","—","—"]
[null,"TC internal Master/Slave ","•","•","•","•","•","•","•","•","•","—","•"]
[null,"1588v2 PTP with two step clock","•","•","•","•","•","•","•","•","•","—","•"]
[null,"1588v2 PTP with one step clock","•","•","•","•","•","•","•","•","•","—","•"]
[null,"Network Time Protocol ","•","•","•","•","•","•","•","•","•","•","•"]
[null,"G.781 compliant clock selection algorithm for the platform as a PTP slave","•","•","•","•","•","•","•","•","•","—","•"]
[null,"G.8265.1 BMCA","•","•","•","•","•","•","•","•","•","—","•"]
[null,"G.8275.1 BMCA","•","•","•","•","•","•","•","•","•","—","•"]
[null,"Boundary Clock","•","•","•","•","•","•","•","•","•","—","•"]
[null,"Peer-to-Peer Transparent Clock","•","•","•","•","•","•","•","•","•","—","•"]
[null,"End-to-End Transparent Clock","•","•","•","•","•","•","•","•","•","—","•"]
[null,"PTP Time Interface","•","•","•","•","•","•","•","•","•","—","•"]
[null,"PTP Precision Time Protocol","•","•","•","•","•","•","•","•","•","—","•"]
[null,"NTP Client","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Power Savings"]
[null,"ActiPHY","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Adaptive Fan Control","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Energy Efficient Ethernet (EEE) Power Management","•","•","•","•","•","•","•","•","•","•","•"]
[null,"LED Power Management","•","•","•","•","•","•","•","•","•","•","•"]
[null,"PerfectReach","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Thermal Protection","•","•","•","•","•","•","•","•","•","•","•"]
[null,"PoE"]
[null,"802.3af PoE","—","•","•","—","•","•","—","•","•","•","—"]
[null,"802.3at PoE","—","•","•","—","•","•","—","•","•","•","—"]
[null,"LLDP-MED Reserve Power","—","•","•","—","•","•","—","•","•","•","—"]
[null,"Classification Reserve Power","—","•","•","—","•","•","—","•","•","•","—"]
[null,"Static Power Allocation","—","•","•","—","•","•","—","•","•","•","—"]
[null,"PoE Scheduler","—","•","•","—","•","•","—","•","•","•","—"]
[null,"PoE Link Check","—","•","•","—","•","•","—","•","•","•","—"]
[null,"PoE Power Budget","—","65W","150W","—","370W","740W","—","370W","740W","370W","—"]
[null,"Performance & Capacity"]
[null,"LAG Groups",5,5,5,13,13,13,26,26,26,14,7]
[null,"MLD Groups",1024,1024,1024,1024,1024,1024,1024,1024,1024,1024,1024]
[null,"IGMP Groups",1024,1024,1024,1024,1024,1024,1024,1024,1024,1024,1024]
[null,"Maximum ACLs",512,512,512,512,512,512,512,512,512,512,512]
[null,"Maximum QCLs",256,256,256,256,256,256,256,256,256,256,256]
[null,"Simultaneous ELPS/APS/EPS stances",29,29,29,29,29,29,29,29,29,"—",21]
[null,"MAC Table Entries","16K","16K","16K","32K","32K","32K","32K","32K","32K","32K","32K"]
[null,"Neighbor Discovery Table Size  (IPv6)",256,256,256,"1K","1K","1K","1K","1K","1K","9k","9k"]
[null,"ARP Inspection Table Size",256,256,256,"1K","1K","1K","1k","1k","1K","1k","1k"]
[null,"ARP Table Size",256,256,256,"2K","2K","2K","2K","2K","2K","2K","2K"]
[null,"Unicast IPv4 Routes","1K","1K","1K","4K","4K","4K","4K","4K","4K","18k","18k"]
[null,"Unicast IPv6 Routes",256,256,256,"1K","1K","1K","1K","1K","1K","9k","9k"]
[null,"Layer 3 VLAN Interfaces",128,128,128,128,128,128,128,128,128,128,128]
[null,"Forwarding Rate ","14.88 Mpps","14.88 Mpps","14.88 Mpps","65.47 Mpps","65.47 Mpps","65.47 Mpps","130.95 Mpps","130.95 Mpps","130.95 Mpps","95.23 Mpps","252.97 Mpps"]
[null,"Switching Capacity","20 Gbps","20 Gbps","20 Gbps","88 Gbps","88 Gbps","88 Gbps","176 Gbps","176 Gbps","176 Gbps","128 Gbps","340 Gbps"]
[null,"1G Interface Latency","4.8us","4.8us","4.8us","4.4us","4.4us","4.4us","4.3us","4.3us","4.3us","3.41us","2.14us"]
[null,"10G Interface Latency","—","—","—","2.2us","2.2us","2.2us","2.0us","2.0us","2.0us","1.485us","1.49us"]
[null,"25G Interface Latency","—","—","—","—","—","—","—","—","—","—","1.15us"]
[null,"Physical Specifications"]
[null,"Chassis Dimensions (H x W x D)","1.73 in. x 8.66 in. x 9.53 in. \n(4.4 cm x 22 cm x 24.2 cm)","1.73 in. x 8.66 in. x 9.53 in. \n(4.4 cm x 22 cm x 24.2 cm)","1.73 in. x 8.66 in. x 9.53 in. \n(4.4 cm x 22 cm x 24.2 cm)","1.73 in. x 17.40 in. x 8.3 in. \n(4.4 cm x 44.2 cm x 21.1 cm)","1.73 in. x 17.40 in. x 8.3 in. \n(4.4 cm x 44.2 cm x 21.1 cm)","1.73 in. x 17.40 in. x 8.3 in. \n(4.4 cm x 44.2 cm x 21.1 cm)","1.73 in. x 17.4 in. x 14.76 in. \n(4.4 cm x 44.2 cm x 37.5 cm)","1.73 in. x 17.4 in. x 14.76 in. \n(4.4 cm x 44.2 cm x 37.5 cm)","1.73 in. x 17.4 in. x 14.76 in. \n(4.4cm x 44.2 cm x 37.5 cm)","1.73 in. x 17.40 in. x 8.3 in. \n(4.4 cm x 44.2 cm x 21.1 cm)","1.73 in. x 17.40 in. x 11.81 in. \n(4.4 cm x 44.2 cm x 30.0 cm) "]
[null,"Chassis Weight","4.63 lbs (2.1 Kg)","4.63 lbs (2.1 Kg)","4.63 lbs (2.1 Kg)","8.6 lbs. (3.9 kg)","8.6 lbs. (3.9 kg)","8.6 lbs. (3.9 kg)","12.35 lbs. (5.6 kg)","12.35 lbs. (5.6 kg)","12.35 lbs. (5.6 kg)","8.4 lbs (3.8kg)","8.6 lbs (3.9 Kg)"]
[null,"1G Copper Ethernet ports (10/100/1000Mbps)",8,"8 PoE","8 PoE",24,"24 PoE","24 PoE",48,"48 PoE","48 PoE",24,"—"]
[null,"1G Combo Copper/SFP Ethernet ports (10/100/1000Mbps)",2,2,2,"—","—","—","—","—","—","—","—"]
[null,"2.5G Copper Ethernet Ports (1G/2.5G)","—","—","—","—","—","—","—","—","—","—","—"]
[null,"Multi-Gig Copper Ethernet Ports (1/2.5/5/10G)","—","—","—","—","—","—","—","—","—","—","—"]
[null,"SFP Ethernet Ports","—","—","—","—","—","—","—","—","—","—","—"]
[null,"SFP+ Ethernet Ports ","—","—","—",2,2,2,4,4,4,4,12]
[null,"SFP28 Ethernet Ports ","—","—","—","—","—","—","—","—","—","—",2]
[null,"Flash Size","32MB","32MB","32MB","32MB","32MB","32MB","32MB","32MB","32MB","128MB","128MB"]
[null,"Internal Fan(s)","Fanless","Fanless","Fanless"," 2x Fans"," 2x Fans","3x Fans"," 1x Blower"," 1x Blower"," 1x Blower","2x Fans"," 1x Blower"]
[null,"Mean Time Between Failure (MTBF)","148,233 hrs","148,233 hrs","148,233 hrs","153,570 hrs","153,570 hrs","153,570 hrs","144,663 hrs","144,663 hrs","144,663 hrs","156,577 hrs","101,026 hrs"]
[null,"Micro USB Port ","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Operating Temperature (relative humidity up to 95% non-Condensing)"," 32° to 122°F"," 32° to 122°F"," 32° to 122°F"," 32° to 122°F"," 32° to 122°F"," 32° to 122°F","32° to 122°F","32° to 122°F"," 32° to 122°F"," 32° to 122°F"," 32° to 122°F"]
[null,"Rack Mount Dimensions","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\"","1U, 19\""]
[null,"RAM Size","512MB","512MB","512MB","512MB","512MB","512MB","512MB","512MB","512MB","1GB","2GB"]
[null,"Power"]
[null,"AC Power Supply","100-240 VAC","100-240 VAC","100-240 VAC","100-240 VAC","100-240 VAC","100-240 VAC","100-240 VAC","100-240 VAC","100-240 VAC","100-240 VAC","100-240 VAC"]
[null,"AC Redunandt Power Supply","—","—","—","—","—","—","—","—","—","—","•"]
[null,"Max BTU w/o PoE","TBD",55,55,"TBD",153,181,"TBD",234,255,169,113]
[null,"Max Wattage (with PoE where applicable)","TBD","90W","175W","TBD","455W","900W","TBD","480W","910W","475W","35W"]
[null,"SFP Support"]
[null,"1000BaseLX -- 1310nm SFP (1200481E1)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"1000BaseSX -- 850nm SFP (1200480E1)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"1000BaseSX -- 850nm SFP (1200480F2)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Enhanced 2.5 Gbps Multimode SFP (1200482G1)","—","—","—","•","•","•","•","•","•","•","•"]
[null,"Enhanced 2.5 Gbps Singlemode SFP (1200483G1)","—","—","—","•","•","•","•","•","•","•","•"]
[null,"1000Base-T Ethernet SFP (1200485G1)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"10GBase-SR SFP+ Transceiver (1700485F1)","—","—","—","•","•","•","•","•","•","•","•"]
[null,"10GBase-LR SFP+ Transceiver (1700486F1)","—","—","—","•","•","•","•","•","•","•","•"]
[null,"SFP+ 10GBASE-T COPPER 30M (1442301F1C)","—","—","—","•","•","•","•","•","•","•","•"]
[null,"SFP SM BIDI SFP 10km (1442110G1, 1442110G2)","TBD","TBD","TBD","TBD","TBD","TBD","TBD","TBD","TBD","TBD","•"]
[null,"SFP SM BIDI SFP 20km (1442120G1, 1442120G2)","TBD","TBD","TBD","TBD","TBD","TBD","TBD","TBD","TBD","TBD","•"]
[null,"SFP GPON ONU STICK FIXED 1G (1442535F3)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"SFP GPON ONU STICK FIXED 2.5G (1442535F2)","—","—","—","•","•","•","•","•","•","•","•"]
[null,"1M Interconnect Cable SFP+ (1710484F1)","—","—","—","•","•","•","•","•","•","•","•"]
[null,"3M Interconnect Cable SFP+ (1710484F3)","—","—","—","•","•","•","•","•","•","•","•"]
[null,"5M Interconnect Cable SFP+ (1710484F5)","—","—","—","•","•","•","•","•","•","•","•"]
[null,"SFP28 SR (1700487F1)","—","—","—","—","—","—","—","—","—","—","•"]
[null,"SFP28 LR (1700488F1)","—","—","—","—","—","—","—","—","—","—","•"]
[null,"1M SFP28 DAC, Interconnect Cable (1700489F1)","—","—","—","—","—","—","—","—","—","—","•"]
[null,"MIB Support "]
[null,"IEEE 802.1 MSTP MIB","•","•","•","•","•","•","•","•","•","•","•"]
[null,"IEEE 802.1AB LLDP-MIB (LLDP MIB included in a clause of the STD)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"IEEE 802.1Q Bridge MIB 2008","•","•","•","•","•","•","•","•","•","•","•"]
[null,"IEEE 802.1X (PAE MIB included in a clause of the STD)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"IEEE 802.3ad (LACP MIB included in a clause of the STD)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"Private MIB framework","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 1213 MIB II","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 1215 TRAPS MIB","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 1850 OSPF Version 2 MIB","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 2674 VLAN MIB","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 2819 RMON (Group 1, 2. 3 & 9)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 2863 Interface Group MIB using SMI v2","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 3621 LLDP-MED Power (POE) (No specific MIB for POE+ exists)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 3635 Ethernet-like MIB","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 3636 802.3 MAU MIB","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 4133 Entity MIB version 3","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 4188 Bridge MIB","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 4292 IP Forwarding Table MIB","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 4293 Management Information Base for the Internet Protocol (IP)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 4668 RADIUS auth. Client MIB","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 4670 RADIUS Accounting MIB","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 4878 Link OAM MIB","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 5519 Multicast Group Membership Discovery MIB","•","•","•","•","•","•","•","•","•","•","•"]
[null,"TIA 1057 LLDP-MED ( MIB is part of the STD)","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 3411 SNMP Management Frameworks","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 3414 User-based Security Model for SNMPv3","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 3415 View-based access Control Model for SNMP","•","•","•","•","•","•","•","•","•","•","•"]
[null,"SNMP MIB OID","•","•","•","•","•","•","•","•","•","•","•"]
[null,"RFC 2613 SMON - PortCopy","•","•","•","•","•","•","•","•","•","•","•"]